For 1990-2009 cars

Connector 1: | X100 Engine Harness to Body Harness
Connector 2: | X107 Left Fog Lamp/Daytime Running Lamp Harness to Forward Lamp Harness (W49 or WDA)
Connector 3: | X108 Right Fog Lamp/Daytime Running Lamp Harness to Forward Lamp Harness (W49 or WDA)
Connector 4: | X109 Instrument Panel Harness to Engine Harness (XA7)
Connector 5: | X111 Engine Harness to Instrument Panel Harness
Connector 6: | X115 Engine Harness to Forward Lamp Harness (TSH)
Connector 7: | X116 Prewired Engine Harness to Fuel Injector Harness (LLT)
Connector 8: | X117 Engine Harness to Prewired Engine Harness (LLT)
Connector 9: | X120 Body Harness to Forward Lamp Harness
Connector 10: | X122 Forward Lamp Harness to Right Park Lamp Harness (X88)
Connector 11: | X123 Forward Lamp Harness to Left Park Lamp Harness (X88)
Connector 12: | X150 Forward Lamp Harness to Right Headlamp Harness (W49 without TSH)
Connector 13: | X150 Forward Lamp Harness to Right Headlamp Harness (W49 with TSH)
Connector 14: | X150 Forward Lamp Harness to Right Headlamp Harness (WDA with TVD)
Connector 15: | X150 Forward Lamp Harness to Right Headlamp Harness (WDA without TVD)
Connector 16: | X150 Forward Lamp Harness to Right Headlamp Harness (X88)
Connector 17: | X150 Forward Lamp Harness to Right Headlamp Harness (Z88 without TVD)
Connector 18: | X150 Right Headlamp Harness to Forward Lamp Harness (Z88 with TVD)
Connector 19: | X151 Forward Lamp Harness to Left Headlamp Harness (W49 without TSH)
Connector 20: | X151 Forward Lamp Harness to Left Headlamp Harness (W49 with TSH)
Connector 21: | X151 Forward Lamp Harness to Left Headlamp Harness (WDA with TVD)
Connector 22: | X151 Forward Lamp Harness to Left Headlamp Harness (WDA without TVD)
Connector 23: | X151 Forward Lamp Harness to Left Headlamp Harness (X88)
Connector 24: | X151 Forward Lamp Harness to Left Headlamp Harness (Z88 without TVD)
Connector 25: | X151 Left Headlamp Harness to Forward Lamp Harness (Z88 with TVD)
Connector 26: | X200 Body Harness to Instrument Panel Harness
Connector 27: | X201 Instrument Panel Harness to Steering Column Harness
Connector 28: | X202 Body Harness to Instrument Panel Harness
Connector 29: | X203 Body Harness to Instrument Panel Harness
Connector 30: | X205 Body Harness to Instrument Panel Harness (N38)
Connector 31: | X209 Body Harness to Trailer Brake Harness (V92)
Connector 32: | X211 Body Harness to Steering Column Harness
Connector 33: | X214 Instrument Panel Harness to HVAC Harness
Connector 34: | X216 Instrument Panel Harness to Headliner Harness (U42)
Connector 35: | X240 Instrument Panel Harness to Floor Console Harness
Connector 36: | X252 Body Harness to Instrument Panel Harness
Connector 37: | X305 Fuel Tank Harness to Body Harness
Connector 38: | X308 Rear Chassis Harness to Fuel Tank Harness
Connector 39: | X314 Body Harness to Passenger Seat Harness
Connector 40: | X315 Body Harness to Driver Seat Harness
Connector 41: | X320 Headliner Harness to Body Harness (DNP or UD7 or UE1)
Connector 42: | X322 Body Harness to Headliner Harness
Connector 43: | X324 Battery Negative Cable Harness to Body Harness
Connector 44: | X325 Battery Positive Cable Harness to Body Harness (UE1)
Connector 45: | X332 Body Harness to Passenger Seat SIR Jumper Harness
Connector 46: | X333 Body Harness to Driver Seat SIR Jumper Harness
Connector 47: | X340 Floor Console Harness to Body Harness
Connector 48: | X341 Floor Console Harness to A/T Shifter Harness
Connector 49: | X343 Headliner Harness to Overhead Console Harness
Connector 50: | X351 Rear HVAC Harness to Body Harness
Connector 51: | X380 Body Harness to Auxiliary Power Outlet - Rear Console Harness (DK1)
Connector 52: | X398 Headliner Harness to Sunroof Harness (C3U)
Connector 53: | X405 Rear Chassis Harness to Body Harness
Connector 54: | X440 Body Harness to Rear Bumper Harness (UD7 or X88)
Connector 55: | X442 Body Harness to Trailer Harness (V92)
Connector 56: | X450 Body Harness to Right Tail Lamp Harness (W49 or X88)
Connector 57: | X450 Body Harness to Right Tail Lamp Harness (WDA)
Connector 58: | X451 Body Harness to Left Tail Lamp Harness (W49 or X88)
Connector 59: | X451 Body Harness to Left Tail Lamp Harness (WDA)
Connector 60: | X500 Driver Door Harness to Body Harness
Connector 61: | X553 Driver Door Trim Panel Harness to Driver Door Harness
Connector 62: | X555 Driver Door Trim Panel Harness to Driver Door Harness
Connector 63: | X600 Passenger Door Harness to Body Harness
Connector 64: | X664 Passenger Door Trim Panel Harness to Passenger Door Harness
Connector 65: | X666 Passenger Door Trim Panel Harness to Passenger Door Harness
Connector 66: | X700 Left Rear Door Harness to Body Harness
Connector 67: | X800 Right Rear Door Harness to Body Harness
Connector 68: | X901 Body Harness to Liftgate Harness
Connector 69: | X902 Body Harness to Liftgate Harness (UVC)
Connector 70: | X903 Body Harness to Liftgate Harness
Connector 71: | X911 Liftgate Harness to Center High Mounted Stop Lamp (CHMSL) Harness
Connector 72: | X920 Liftgate Harness to Liftgate Applique Harness (W49 or Z88)
Connector 73: | X931 Liftgate Harness to Liftgate Applique Harness (W49 or Z88)
Connector 74: | X933 License Lamp Harness to Liftgate Harness (without X88)
Connector 75: | X940 Liftgate Harness to Liftgate Trim Panel Harness

### X100 Engine Harness to Body Harness

#### Connector Part Information

- OEM: 19177608
- Service: 19180282
- Description: 16-Way F GT150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177609
- Service: 15306364
- Description: 16-Way M GT150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191818/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)(GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X100 Engine Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 PU | 1589 | Fuel Level Sensor Signal | A | 0.5 PU | 1589 | Fuel Level Sensor Signal
B | 0.35 TN | 2759 | Low Reference | B | 0.5 TN | 2759 | Low Reference
C | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal | C | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
D | 0.5 WH | 883 | Low Reference | D | 0.5 WH | 883 | Low Reference
E | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal | E | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
F | 0.5 OG | 885 | Low Reference | F | 0.5 OG | 885 | Low Reference
G | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal | G | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
H | 0.35 GY | 2709 | 5-Volt Reference | H | 0.5 GY | 2709 | 5-Volt Reference
J | 0.5 L-BU | 2088 | Low Reference | J | 0.5 L-BU | 2088 | Low Reference
K | 0.5 D-GN | 2087 | 5-Volt Reference | K | 0.5 D-GN | 2087 | 5-Volt Reference
L | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control | L | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control
M | 0.35 PK | 439 | Ignition Voltage | M | 0.35 PK | 439 | Ignition Voltage
N | 1 OG | 1470 | Brake Booster Pump Motor Voltage | N | 1 OG | 1470 | Brake Booster Pump Motor Voltage
P-S | -- | -- | Not Used | P-S | -- | -- | Not Used

### X107 Left Fog Lamp/Daytime Running Lamp Harness to Forward Lamp Harness (W49 or WDA)

#### Connector Part Information

- OEM: 7283-5541-30
- Service: See Catalog
- Description: 3-Way F1.5 Series, Sealed (BK)

#### Connector Part Information

- OEM: 7282-5541-30
- Service: See Catalog
- Description: 3-Way M 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 3
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 1, 2
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X107 Left Fog Lamp/Daytime Running Lamp Harness to Forward Lamp Harness (W49 or WDA)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BK | 1350 | Ground | 1 | 1 BK | 1350 | Ground
2 | 1 L-BU/WH | 1314 | Left Daytime Running Lamp Voltage (T61) | 2 | 0.5 PU | 359 | Left Daytime Running Lamp Voltage (T61)
3 | 0.5 PU | 34 | Front Fog Lamp Voltage (T96) | 3 | 0.5 PU | 34 | Front Fog Lamp Voltage (T96)

### X108 Right Fog Lamp/Daytime Running Lamp Harness to Forward Lamp Harness (W49 or WDA)

#### Connector Part Information

- OEM: 7283-5541-30
- Service: See Catalog
- Description: 3-Way F 1.5 YESC Series, Sealed (BK)

#### Connector Part Information

- OEM: 7282-5541-30
- Service: See Catalog
- Description: 3-Way M 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 3
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1, 2
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 3
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X108 Right Fog Lamp/Daytime Running Lamp Harness to Forward Lamp Harness (W49 or WDA)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BK | 1350 | Ground | 1 | 1 BK | 1250 | Ground
2 | 1 D-BU/WH | 1315 | Right Daytime Running Lamp Voltage (T61) | 2 | 0.35 PU | 359 | Right Daytime Running Lamp Voltage (T61)
3 | 0.5 PU | 34 | Front Fog Lamp Voltage (T96) | 3 | 0.5 PU | 34 | Front Fog Lamp Voltage (T96)

### X109 Instrument Panel Harness to Engine Harness (XA7)

#### Connector Part Information

- OEM: 7123-4210-30
- Service: See Catalog
- Description: 1-Way F 375 Series, Sealed (BK)

#### Connector Part Information

- OEM: 7222-4210-30
- Service: See Catalog
- Description: 1-Way M 058Y/375 PBT, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-3250/10
- Core/Insulation Crimp: G/3
- Release Tool/Test Probe: 12094430/J-35616-22 (RD)

#### Terminal Part Information

- Terminal/Tray: 7114-3250/14
- Core/Insulation Crimp: G/3
- Release Tool/Test Probe: 12094430/J-35616-21 (RD)

#### X109 Instrument Panel Harness to Engine Harness (XA7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 5 RD/WH | 1440 | Battery Positive Voltage | 1 | 5 RD/WH | 1440 | Battery Positive Voltage

### X111 Engine Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: 19177608
- Service: 15306381
- Description: 16-Way F GT 150 Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 19177609
- Service: 15306364
- Description: 16-Way M 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: F-G, M : 2/A
- Core/Insulation Crimp: Pins: A-E, H, J-L, N, P, R-S : E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: F-G, M : E/1
- Core/Insulation Crimp: Pins: A-E, H, J-L, N, P, R-S : E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X111 Engine Harness to Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-BU | 1161 | APP Sensor 1 Signal | A | 0.35 D-BU | 1161 | APP Sensor 1 Signal
B | 0.5 L-BU | 1162 | APP Sensor 2 Signal | B | 0.35 L-BU | 1162 | APP Sensor 2 Signal
C | 0.5 WH/BK | 1164 | 5-Volt Reference | C | 0.35 WH/BK | 1164 | 5-Volt Reference
D | 0.5 BN | 1271 | Low Reference | D | 0.35 BN | 1271 | Low Reference
E | 0.5 PU | 1272 | Low Reference | E | 0.35 PU | 1272 | Low Reference
F | 1 PU | 92 | Windshield Wiper Motor High Speed | F | 1 PU | 92 | Windshield Wiper Motor High Speed
G | 1 D-GN | 95 | Windshield Washer Switch Signal | G | 1 D-GN | 95 | Windshield Washer Switch Signal
H | 0.5 TN | 1274 | 5-Volt Reference | H | 0.35 TN | 1274 | 5-Volt Reference
J | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | J | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
K | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | K | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
L | 0.5 BN/WH | 419 | MIL Control | L | 0.35 BN/WH | 419 | MIL Control
M | 1 BK | 1650 | Ground | M | 1 BK | 1650 | Ground
N | 0.5 TN/WH | 6433 | CAN Bus High Serial Data | N | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
P | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data | P | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
R | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (U3R or UVB or UZR) | R | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (U3R or UVB or UZR)
S | 0.5 L-BU | 5986 | Communication Enable | S | 0.35 L-BU | 5986 | Communication Enable

### X115 Engine Harness to Forward Lamp Harness (TSH)

#### Connector Part Information

- OEM: 7283-5553-30
- Service: 88988392
- Description: 6-Way F YESC/USCAR Class III, Sealed (BK)

#### Connector Part Information

- OEM: 7282-5553-30
- Service: 88988399
- Description: 6-Way M YESC/USCAR Class III, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X115 Engine Harness to Forward Lamp Harness (TSH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 1 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
2 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | 2 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
3 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 3 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
4 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | 4 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
5 | 0.5 L-BU | 5986 | Communication Enable | 5 | 0.5 L-BU | 5986 | Communication Enable
6 | 0.5 RD/WH | 4440 | Battery Positive Voltage | 6 | 0.5 RD/WH | 4440 | Battery Positive Voltage

### X116 Prewired Engine Harness to Fuel Injector Harness (LLT)

#### Connector Part Information

- OEM: 33472-0606
- Service: See Catalog
- Description: 6-Way F MX150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 33482-0601
- Service: See Catalog
- Description: 6-Way M MX150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 33012-1002/26
- Core/Insulation Crimp: 2/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X116 Prewired Engine Harness to Fuel Injector Harness (LLT)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2 | 1 | 1 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
2 | 1 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Cylinder 2 | 2 | 1 BK | 4902 | Direct Fuel Injector (DFI) High Voltage Cylinder 2
3 | 1 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4 | 3 | 1 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
4 | 1 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Cylinder 4 | 4 | 1 BK | 4904 | Direct Fuel Injector (DFI) High Voltage Cylinder 4
5 | 1 PU | 4806 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 6 | 5 | 1 TN | 4806 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 6
6 | 1 PU/WH | 4906 | Direct Fuel Injector (DFI) High Voltage Cylinder 6 | 6 | 1 BK | 4906 | Direct Fuel Injector (DFI) High Voltage Cylinder 6

### X117 Engine Harness to Prewired Engine Harness (LLT)

#### Connector Part Information

- OEM: 33472-1236
- Service: See Catalog
- Description: 12-Way F MX150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 33482-1216
- Service: See Catalog
- Description: 12-Way M MX150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 33012-1002/26
- Core/Insulation Crimp: 2/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X117 Engine Harness to Prewired Engine Harness (LLT)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 1 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1 | 2 | 1 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
3 | 1 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3 | 3 | 1 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
4 | 1 L-GN | 4805 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 5 | 4 | 1 TN | 4805 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 5
5 | 0.5 TN | 808 | Low Reference | 5 | 0.5 L-BU | 808 | Low Reference
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | 1 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Cylinder 1 | 8 | 1 BK | 4901 | Direct Fuel Injector (DFI) High Voltage Cylinder 1
9 | 1 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Cylinder 3 | 9 | 1 BK | 4903 | Direct Fuel Injector (DFI) High Voltage Cylinder 3
10 | 1 L-GN/WH | 4905 | Direct Fuel Injector (DFI) High Voltage Cylinder 5 | 10 | 1 BK | 4905 | Direct Fuel Injector (DFI) High Voltage Cylinder 5
11 | 0.35 GY | 598 | 5-Volt Reference | 11 | 0.35 WH | 598 | 5-Volt Reference
12 | 0.5 YE | 2918 | FRP Sensor Signal | 12 | 0.5 BK | 2918 | FRP Sensor Signal

### X120 Body Harness to Forward Lamp Harness

#### Connector Part Information

- OEM: 7283-5574-10
- Service: See Catalog
- Description: 8-Way F 2.8 Series, Sealed (D-GY)

#### Connector Part Information

- OEM: 7282-5574-10
- Service: See Catalog
- Description: 8-Way M 2.8 Series, Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4150-02/9
- Core/Insulation Crimp: Pins: 1-6 : E/1
- Core/Insulation Crimp: Pins: 8 : See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X120 Body Harness to Forward Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal | 1 | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal
2 | 0.35 GY | 5600 | Low Reference | 2 | 0.35 GY | 5600 | Low Reference
3 | 0.35 YE | 61 | Low Reference | 3 | 0.35 YE | 61 | Low Reference
4 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal | 4 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
5 | 0.35 YE | 354 | Discriminating Sensor - Signal | 5 | 0.35 YE | 354 | Discriminating Sensor - Signal
6 | 0.35 TN/OG | 5045 | Front End Sensor - Signal | 6 | 0.35 TN/OG | 5045 | Front End Sensor - Signal
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | 3 RD | 1342 | Battery Positive Voltage (TB5) | 8 | 2 RD/BK | 1342 | Battery Positive Voltage (TB5)

### X122 Forward Lamp Harness to Right Park Lamp Harness (X88)

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177532
- Service: 15326813
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: 2/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X122 Forward Lamp Harness to Right Park Lamp Harness (X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-BU/WH | 1315 | Right Turn Lamp Voltage | A | 0.8 GN | -- | Right Turn Lamp Voltage
B | 0.5 BK | 1250 | Ground | B | 0.8 BK | -- | Ground
C | 0.5 BN/WH | 309 | Right Park Lamp Voltage | C | 0.8 RD | -- | Right Park Lamp Voltage

### X123 Forward Lamp Harness to Left Park Lamp Harness (X88)

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177532
- Service: 15326813
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: 2/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X123 Forward Lamp Harness to Left Park Lamp Harness (X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU/WH | 1314 | Left Turn Lamp Voltage | A | 0.8 GN | -- | Left Turn Lamp Voltage
B | 0.5 BK | 1350 | Ground | B | 0.8 BK | -- | Ground
C | 0.5 PU/WH | 709 | Left Park Lamp Voltage | C | 0.8 RD | -- | Left Park Lamp Voltage

### X150 Forward Lamp Harness to Right Headlamp Harness (W49 without TSH)

#### Connector Part Information

- OEM: 88986902
- Service: 19151498
- Description: 5-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177549
- Service: 89046648
- Description: 5-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, B, D, E: E/A
- Core/Insulation Crimp: Pin: C : 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A, C, D: E/1
- Core/Insulation Crimp: Pins: B, E: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X150 Forward Lamp Harness to Right Headlamp Harness (W49 without TSH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage | A | 0.8 GN | -- | Right Turn Signal Indicator Lamp Voltage
B | 0.5 BN/WH | 309 | Right Park Lamp Voltage | B | 0.5 BU | -- | Right Park Lamp Voltage
C | 1 TN/WH | 312 | Right Headlamp Low Beam Voltage | C | 0.8 PU | -- | Right Headlamp Low Beam Voltage
D | 0.5 BK | 1250 | Ground | D | 1 BK | -- | Ground
E | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage | E | 0.35 GY | -- | Right Headlamp High Beam Voltage

### X150 Forward Lamp Harness to Right Headlamp Harness (W49 with TSH)

#### Connector Part Information

- OEM: 88986324
- Service: 88986261
- Description: 14-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177606
- Service: 88986246
- Description: 14-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, B, D-P: E/A
- Core/Insulation Crimp: Pin: C : 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A, B, D-P: E/4
- Core/Insulation Crimp: Pins: C: E/1
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X150 Forward Lamp Harness to Right Headlamp Harness (W49 with TSH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 RD/BU | 7308 | Battery Positive Voltage | A | 0.35 RD | -- | Battery Positive Voltage
B | 0.5 RD/WH | 4440 | Battery Positive Voltage | B | 0.5 RD | -- | Battery Positive Voltage
C | 1 TN/WH | 312 | Right Headlamp Low Beam Voltage | C | 0.8 PU | -- | Right Headlamp Low Beam Voltage
D | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage | D | 0.35 GY | -- | Right Headlamp High Beam Voltage
E | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus- | E | 0.35 WH | -- | High Speed GMLAN Serial Data Bus-
F | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | F | 0.35 YE | -- | High Speed GMLAN Serial Data Bus+
G | 0.5 BK | 1250 | Ground | G | 0.5 BK | -- | Ground
H | 0.5 L-GN/BK | 1315 | Right Turn Signal Indicator Lamp Voltage | H | 0.8 GN | -- | Right Turn Signal Indicator Lamp Voltage
J | 0.5 PU | 309 | Right Turn Signal Indicator Lamp Voltage | J | 0.5 BU | -- | Right Turn Signal Indicator Lamp Voltage
K | 0.5 L-BU | 5986 | Communication Enable | K | 0.35 RD | -- | Communication Enable
L | 0.35 D-GN | 6134 | Linear Interconnect Network (LIN) | L | 0.35 OG | -- | Linear Interconnect Network (LIN)
M-N | -- | -- | Not Used | M-N | -- | -- | Not Used
P | 0.5 BK | 1250 | Ground | P | 1 BK | -- | Ground

### X150 Forward Lamp Harness to Right Headlamp Harness (WDA with TVD)

#### Connector Part Information

- OEM: 19177571
- Service: 88986254
- Description: 8-Way F GT 280 Sealed 5.8 (BK)

#### Connector Part Information

- OEM: 19177573
- Service: 15306424
- Description: 8-Way M GT 280 Sealed 5.8 (BK)

#### Terminal Part Information

- Pins: A-H
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: Pins: G-H : 2/5
- Core/Insulation Crimp: Pins: A-F : E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X150 Forward Lamp Harness to Right Headlamp Harness (WDA with TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 1250 | Ground | A | 0.5 BK | -- | Ground
B | 0.5 BN/WH | 309 | Right Turn Signal Indicator Lamp Voltage | B | 0.5 PU | -- | Right Park Lamp Voltage
C | 0.5 BK | 1250 | Ground | C | 0.5 BK | -- | Ground
D | 0.5 PU | 359 | DRL Voltage | D | 0.5 PU | -- | DRL Voltage
E | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage | E | 0.5 GN/WH | -- | Right Headlamp High Beam Voltage
F | 0.5 BK | 1250 | Ground | F | -- | -- | Not Used
G | 1 TN/WH | 312 | Right Headlamp Low Beam Voltage | G | 0.8 YE | -- | Right Headlamp Low Beam Voltage
H | 1 BK | 1250 | Ground | H | 0.8 BK | -- | Ground

### X150 Forward Lamp Harness to Right Headlamp Harness (WDA without TVD)

#### Connector Part Information

- OEM: 19177555
- Service: 88953154
- Description: 6-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 19177557
- Service: 15326640
- Description: 6-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X150 Forward Lamp Harness to Right Headlamp Harness (WDA without TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage | A | 0.5 GN/WH | -- | Right Headlamp High Beam Voltage
B | 0.5 TN/WH | 312 | Right Headlamp Low Beam Voltage | B | 0.5 YE | -- | Right Headlamp Low Beam Voltage
C | 0.5 BK | 1250 | Ground | C | 0.5 BK | -- | Ground
D | 0.5 BK | 1250 | Ground | D | 0.5 BK | -- | Ground
E | 0.5 BK | 1250 | Ground | E | 0.5 BK | -- | Ground
F | 0.5 BN/WH | 309 | Right Park Lamp Voltage | F | 0.5 PU | -- | Right Park Lamp Voltage

### X150 Forward Lamp Harness to Right Headlamp Harness (X88)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Service: See Catalog
- Description: 4-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X150 Forward Lamp Harness to Right Headlamp Harness (X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage | A | 1.25 BK | -- | Right Headlamp High Beam Voltage
B | 0.5 BK | 1250 | Ground | B | 1.25 BK | -- | Ground
C | 0.5 TN/WH | 312 | Right Headlamp Low Beam Voltage | C | 1.25 RD | -- | Right Headlamp Low Beam Voltage
D | 0.5 BK | 1250 | Ground | D | 1.25 RD | -- | Ground

### X150 Forward Lamp Harness to Right Headlamp Harness (Z88 without TVD)

#### Connector Part Information

- OEM: 19177555
- Service: 88953154
- Description: 6-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 19177557
- Service: 15326640
- Description: 6-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X150 Forward Lamp Harness to Right Headlamp Harness (Z88 without TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage | A | 1.5 WH | -- | Right Headlamp High Beam Voltage
B | 0.5 TN/WH | 312 | Right Headlamp Low Beam Voltage | B | 1.5 RD | -- | Right Headlamp Low Beam Voltage
C | 0.5 BN/WH | 309 | Right Park Lamp Voltage | C | 0.8 BU | -- | Right Park Lamp Voltage
D | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage | D | 0.8 YE | -- | Right Turn Signal Indicator Lamp Voltage
E | 0.5 BK | 1250 | Ground | E | 2 BK | -- | Ground
F | -- | -- | Not Used | F | -- | -- | Not Used

### X150 Right Headlamp Harness to Forward Lamp Harness (Z88 with TVD)

#### Connector Part Information

- OEM: 7283-5574-10
- Service: 88987869
- Description: 8-Way F 2.8 Series, Sealed (D-GY)

#### Connector Part Information

- OEM: 7282-5574-10
- Service: See Catalog
- Description: 8-Way M 2.8 Series, Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 2
- Terminal/Tray: 7114-4151-02/9
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1, 3-6
- Terminal/Tray: 7114-4150-02/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X150 Right Headlamp Harness to Forward Lamp Harness (Z88 with TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.5 WH | -- | Right Headlamp High Beam Voltage | 1 | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Voltage
2 | 0.8 RD | -- | Right Headlamp Low Beam Voltage | 2 | 1 TN/WH | 312 | Right Headlamp Low Beam Voltage
3 | 0.8 YE | -- | Right Turn Signal Indicator Lamp Voltage | 3 | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage
4 | 0.8 BU | -- | Right Park Lamp Voltage | 4 | 0.5 BN/WH | 309 | Right Park Lamp Voltage
5 | 0.8 OG | -- | Right DRL/Turn Voltage | 5 | 0.5 D-GN | 5365 | Right DRL/Turn Voltage
6 | 2 BK | -- | Ground | 6 | 0.5 BK | 1250 | Ground
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used

### X151 Forward Lamp Harness to Left Headlamp Harness (W49 without TSH)

#### Connector Part Information

- OEM: 88986902
- Service: 19151498
- Description: 5-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177549
- Service: 89046648
- Description: 5-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, B, D, E: E/A
- Core/Insulation Crimp: Pin: C : 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A, C, D: E/1
- Core/Insulation Crimp: Pins: B, E: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X151 Forward Lamp Harness to Left Headlamp Harness (W49 without TSH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage | A | 0.8 GN | -- | Left Turn Signal Indicator Lamp Voltage
B | 0.5 PU | 709 | Left Park Lamp Voltage | B | 0.5 BU | -- | Left Park Lamp Voltage
C | 1 YE | 712 | Left Headlamp Low Beam Voltage | C | 0.8 PU | -- | Left Headlamp Low Beam Voltage
D | 0.5 BK | 1350 | Ground | D | 1 BK | -- | Ground
E | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage | E | 0.35 GY | -- | Left Headlamp High Beam Voltage

### X151 Forward Lamp Harness to Left Headlamp Harness (W49 with TSH)

#### Connector Part Information

- OEM: 19177566
- Service: 15326835
- Description: 8-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177568
- Service: See Catalog
- Description: 8-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, C, D, F-H: E/A
- Core/Insulation Crimp: Pin: B, E: 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A, C, D, F-H: E/4
- Core/Insulation Crimp: Pins: B, E: E/1
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X151 Forward Lamp Harness to Left Headlamp Harness (W49 with TSH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 RD/BU | 7308 | Battery Positive Voltage | A | 0.35 RD | -- | Battery Positive Voltage
B | 1 YE | 712 | Left Headlamp Low Beam Voltage | B | 0.8 PU | -- | Left Headlamp Low Beam Voltage
C | 0.5 PU | 709 | Left Turn Signal Indicator Lamp Voltage | C | 0.5 BU | -- | Left Turn Signal Indicator Lamp Voltage
D | 0.5 BK | 1350 | Ground | D | 0.35 BK | -- | Ground
E | 1 BK | 1350 | Ground | E | 1 BK | -- | Ground
F | 0.35 D-GN | 6134 | Linear Interconnect Network (LIN) | F | 0.35 OG | -- | Linear Interconnect Network (LIN)
G | 0.5 D-GN/WH | 1314 | Left Turn Signal Indicator Lamp Voltage | G | 0.8 GN | -- | Left Turn Signal Indicator Lamp Voltage
H | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage | H | 0.35 GY | -- | Left Headlamp High Beam Voltage

### X151 Forward Lamp Harness to Left Headlamp Harness (WDA with TVD)

#### Connector Part Information

- OEM: 19177571
- Service: 88986254
- Description: 8-Way F GT 280 Sealed 5.8 (BK)

#### Connector Part Information

- OEM: 19177573
- Service: 15306424
- Description: 8-Way M GT 280 Sealed 5.8 (BK)

#### Terminal Part Information

- Pins: A-H
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: Pins: G-H : 2/5
- Core/Insulation Crimp: Pins: A-F : E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X151 Forward Lamp Harness to Left Headlamp Harness (WDA with TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 1350 | Ground | A | 0.5 BK | -- | Ground
B | 0.5 PU | 709 | Left Park Lamp Voltage | B | 0.5 PU | -- | Left Park Lamp Voltage
C | 0.5 BK | 1350 | Ground | C | 0.5 BK | -- | Ground
D | 0.5 PU | 359 | DRL Voltage | D | 0.5 PU | -- | DRL Voltage
E | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage | E | 0.5 GN/WH | -- | Left Headlamp High Beam Voltage
F | 0.5 BK | 1350 | Ground | F | -- | -- | Not Used
G | 1 YE | 712 | Left Headlamp Low Beam Voltage | G | 0.8 YE | -- | Left Headlamp Low Beam Voltage
H | 1 BK | 1350 | Ground | H | 0.8 BK | -- | Ground

### X151 Forward Lamp Harness to Left Headlamp Harness (WDA without TVD)

#### Connector Part Information

- OEM: 19177555
- Service: 88953154
- Description: 6-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 19177557
- Service: 15326640
- Description: 6-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X151 Forward Lamp Harness to Left Headlamp Harness (WDA without TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage | A | 0.5 GN/WH | -- | Left Headlamp High Beam Voltage
B | 0.5 YE | 712 | Left Headlamp Low Beam Voltage | B | 0.5 YE | -- | Left Headlamp Low Beam Voltage
C | 0.5 BK | 1350 | Ground | C | 0.5 BK | -- | Ground
D | 0.5 BK | 1350 | Ground | D | 0.5 BK | -- | Ground
E | 0.5 BK | 1350 | Ground | E | 0.5 BK | -- | Ground
F | 0.5 PU | 709 | Left Park Lamp Voltage | F | 0.5 PU | -- | Left Park Lamp Voltage

### X151 Forward Lamp Harness to Left Headlamp Harness (X88)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Service: See Catalog
- Description: 4-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X151 Forward Lamp Harness to Left Headlamp Harness (X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage | A | 1.25 BK | -- | Left Headlamp High Beam Voltage
B | 0.5 BK | 1350 | Ground | B | 1.25 BK | -- | Ground
C | 0.5 YE | 712 | Left Headlamp Low Beam Voltage | C | 1.25 RD | -- | Left Headlamp Low Beam Voltage
D | 0.5 BK | 1350 | Ground | D | 1.25 RD | -- | Ground

### X151 Forward Lamp Harness to Left Headlamp Harness (Z88 without TVD)

#### Connector Part Information

- OEM: 19177555
- Service: 88953154
- Description: 6-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326640
- Service: 15326640
- Description: 6-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A-E
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: Pins: B : 2/5
- Core/Insulation Crimp: Pins: A, C-E : E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X151 Forward Lamp Harness to Left Headlamp Harness (Z88 without TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage | A | 1.5 WH | -- | Left Headlamp High Beam Voltage
B | 0.8 YE | 712 | Left Headlamp Low Beam Voltage | B | 1.5 RD | -- | Left Headlamp Low Beam Voltage
C | 0.5 PU | 709 | Left Park Lamp Voltage | C | 0.8 BU | -- | Left Park Lamp Voltage
D | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage | D | 0.8 YE | -- | Left Turn Signal Indicator Lamp Voltage
E | 0.5 BK | 1350 | Ground | E | 2 BK | -- | Ground
F | -- | -- | Not Used | F | -- | -- | Not Used

### X151 Left Headlamp Harness to Forward Lamp Harness (Z88 with TVD)

#### Connector Part Information

- OEM: 7283-5574-10
- Service: 88987869
- Description: 8-Way F 2.8 Series, Sealed (D-GY)

#### Connector Part Information

- OEM: 7282-5574-10
- Service: See Catalog
- Description: 8-Way M 2.8 Series, Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 2
- Terminal/Tray: 7114-4151-02/9
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1-6
- Terminal/Tray: 7114-4150-02/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 8
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X151 Left Headlamp Harness to Forward Lamp Harness (Z88 with TVD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.5 WH | -- | Left Headlamp High Beam Voltage | 1 | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Voltage
2 | 0.8 RD | -- | Left Headlamp Low Beam Voltage | 2 | 1 YE | 712 | Left Headlamp Low Beam Voltage
3 | 0.8 YE | -- | Left Turn Signal Indicator Lamp Voltage | 3 | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage
4 | 0.8 BU | -- | Left Park Lamp Voltage | 4 | 0.5 PU | 709 | Left Park Lamp Voltage
5 | 0.8 OG | -- | Left DRL/Turn Voltage | 5 | 0.5 D-BU | 5364 | Left DRL/Turn Voltage
6 | 2 BK | -- | Ground | 6 | 0.5 BK | 1350 | Ground
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used

### X200 Body Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: 7283-6447-40
- Service: 88956524
- Description: 14-Way F Hybrid Series (L-GY)

#### Connector Part Information

- OEM: 7282-6447-40
- Service: 88956523
- Description: 14-Way M Hybrid Series (L-GY)

#### Terminal Part Information

- Pins: 2, 6, 9-12
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 3-5, 9-10, 22
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 8
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 7, 14
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 8, 14
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: Pins: 8 : E/A
- Core/Insulation Crimp: Pins: 14 : C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 3-5, 9-10
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: Pins: 5, 9-10 : E/A
- Core/Insulation Crimp: Pins: 3-4, 9-10 : C/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 2-4, 6, 9-12
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1, 7
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X200 Body Harness to Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 RD/WH | 2040 | Battery Positive Voltage (UQA or UQS) | 1 | 2 RD/WH | 2040 | Battery Positive Voltage (UQA or UQS)
2 | 0.35 TN | 185 | Low Washer Fluid Indicator Control | 2 | 0.35 TN | 185 | Low Washer Fluid Indicator Control
3 | 0.8 D-GN | 117 | Right Front Speaker Output (-) | 3 | 0.8 D-GN | 117 | Right Front Speaker Output (-) (UQA or UQS)
0.5 D-GN | 117 | Right Front Speaker Output (-) (UQF)
4 | 0.8 L-GN | 200 | Right Front Speaker Output (+) | 4 | 0.8 L-GN | 200 | Right Front Speaker Output (+) (UQA or UQS)
0.5 L-GN | 200 | Right Front Speaker Output (+) (UQF)
5 | 1 BK | 750 | Ground | 5 | 0.8 BK | 750 | Ground
6 | 0.5 L-BU | 2088 | Low Reference | 6 | 0.5 L-BU | 2088 | Low Reference
7 | 3 BK/WH | 351 | Ground (UQA or UQS) | 7 | 3 BK/WH | 351 | Ground (UQA or UQS)
8 | 0.8 OG | 1732 | Courtesy Lamps Voltage | 8 | 0.8 OG | 1732 | Courtesy Lamps Voltage
9 | 0.8 L-BU | 115 | Right Rear Speaker Output (-) (UQA or UQS) | 9 | 0.8 L-BU | 115 | Right Rear Speaker Output (-) (UQA or UQS)
0.5 L-BU | 115 | Right Rear Speaker Output (-) (UQF) | 0.5 L-BU | 115 | Right Rear Speaker Output (-) (UQF)
10 | 0.8 D-BU | 46 | Right Rear Speaker Output (+) (UQA or UQS) | 10 | 0.8 D-BU | 46 | Right Rear Speaker Output (+) (UQA or UQS)
0.5 D-BU | 46 | Right Rear Speaker Output (+) (UQF) | 0.5 D-BU | 46 | Right Rear Speaker Output (+) (UQF)
11 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE) | 11 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE)
12 | 0.5 D-GN | 2087 | 5-Volt Reference | 12 | 0.5 D-GN | 2087 | 5-Volt Reference
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | 2 BK/WH | 351 | Ground | 14 | 1 BK/WH | 351 | Ground

### X201 Instrument Panel Harness to Steering Column Harness

#### Connector Part Information

- OEM: 7283-4190-30
- Service: See Catalog
- Description: 43-Way F YESC Unsealed Series (BK)

#### Connector Part Information

- OEM: 7282-4190-30
- Service: See Catalog
- Description: 43-Way M YESC Unsealed (BK)

#### Terminal Part Information

- Pins: 10, 27, 37-38, 43
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 3, 5
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 8-9, 11-15, 17, 19-26, 28-31, 34-36, 39-40, 42
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 10, 27, 37-38
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 1, 7
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X201 Instrument Panel Harness to Steering Column Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 OG | 2098 | Steering Column Telescope Motor Forward (N38) | 1 | 1 OG | 2098 | Steering Column Telescope Motor Forward (N38)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38) | 3 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 1 PK | 2111 | Steering Column Tilt Motor Control - Up (N38) | 5 | 1 PK | 2111 | Steering Column Tilt Motor Control - Up (N38)
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 1 BN | 2112 | Steering Column Tilt Motor Control - Down (N38) | 7 | 1 BN | 2112 | Steering Column Tilt Motor Control - Down (N38)
8 | 0.35 RD/WH | 1040 | Battery Positive Voltage | 8 | 0.35 RD/WH | 1040 | Battery Positive Voltage
9 | 0.35 PU/WH | 7005 | LED Dimming Signal | 9 | 0.35 PU/WH | 7005 | LED Dimming Signal
10 | 0.5 D-GN | 2087 | 5-Volt Reference | 10 | 0.5 D-GN | 2087 | 5-Volt Reference
0.5 D-GN | 2087 | 5-Volt Reference | 0.5 D-GN | 2087 | 5-Volt Reference
11 | 0.35 PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal (N38) | 11 | 0.35 PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal (N38)
12 | 0.35 BK | 1450 | Ground | 12 | 0.35 BK | 1450 | Ground
13 | 0.35 PU | 5526 | Memory Set Switch Signal | 13 | 0.35 PU | 5526 | Memory Set Switch Signal
14 | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control | 14 | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control
15 | 0.35 L-BU | 553 | Tow/Haul Switch Signal | 15 | 0.35 L-BU | 553 | Tow/Haul Switch Signal
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | 0.35 OG | 2095 | Steering Column Tilt and Telescope Reverse Switch Signal (N38) | 17 | 0.35 OG | 2095 | Steering Column Tilt and Telescope Reverse Switch Signal (N38)
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | 0.35 GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal (N38) | 19 | 0.35 GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal (N38)
20 | 0.35 YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal (N38) | 20 | 0.35 YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal (N38)
21 | 0.35 RD/WH | 1040 | Battery Positive Voltage | 21 | 0.35 RD/WH | 1040 | Battery Positive Voltage
22 | 0.35 TN | 2144 | Hazard Switch Signal | 22 | 0.35 TN | 2144 | Hazard Switch Signal
23 | 0.35 PU | 1375 | 12-Volt Reference | 23 | 0.35 PU | 1375 | 12-Volt Reference
24 | 0.35 GY | 6206 | Low Reference (N38) | 24 | 0.35 GY | 6206 | Low Reference (N38)
25 | 0.35 BK/WH | 1551 | Ground | 25 | 0.35 BK/WH | 1551 | Ground
26 | 0.35 TN | 6207 | 5-Volt Reference (N38) | 26 | 0.35 TN | 6207 | 5-Volt Reference (N38)
27 | 0.5 L-BU | 2088 | Low Reference | 27 | 0.5 L-BU | 2088 | Low Reference
0.5 L-BU | 2088 | Low Reference
28 | 0.35 OG | 2153 | Steering Column Telescope Sensor Signal (N38) | 28 | 0.35 OG | 2153 | Steering Column Telescope Sensor Signal (N38)
29 | 0.35 TN | 28 | Horn Relay Control | 29 | 0.35 TN | 28 | Horn Relay Control
30 | 0.35 OG | 2154 | Steering Column Tilt Sensor Signal (N38) | 30 | 0.35 OG | 2154 | Steering Column Tilt Sensor Signal (N38)
31-35 | -- | -- | Not Used | 32-33 | -- | -- | Not Used
36 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal | 36 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal
37 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data | 37 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
0.5 TN/WH | 6433 | CAN Bus High Serial Data
38 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data | 38 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
39 | 0.35 L-GN | 1011 | Remote Radio Control Signal (RCA) | 39 | 0.35 L-GN | 1011 | Remote Radio Control Signal (RCA)
40 | 0.35 PK | 94 | Windshield Washer Switch Signal (XA7) | 40 | 0.35 PK | 94 | Windshield Washer Switch Signal (XA7)
41 | -- | -- | Not Used | 41 | -- | -- | Not Used
42 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | 42 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
43 | 0.5 RD/WH | 2140 | Battery Positive Voltage (N38) | 43 | 0.5 RD/WH | 2140 | Battery Positive Voltage (N38)

### X202 Body Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: 7283-4192-40
- Service: See Catalog
- Description: 43-Way F YESC Unsealed Series (L-GY)

#### Connector Part Information

- OEM: 7282-4192-40
- Service: See Catalog
- Description: 43-Way M LIF YESC Series (L-GY)

#### Terminal Part Information

- Pins: 2
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 9-23, 25, 27-31, 33-42
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 8, 24
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 1, 32
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: Pins: 1 : C/A
- Core/Insulation Crimp: Pins: 32 : E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 3, 5
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 24
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 32, 1
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: Pins: 32 : E/A
- Core/Insulation Crimp: Pins: 1 : C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 2
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 9-23, 25, 27-31, 33-42
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 3, 5
- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### X202 Body Harness to Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BK | 1450 | Ground | 1 | 1 BK | 1450 | Ground
2 | 0.5 BN | 6555 | Auxiliary Temperature Motor Voltage | 2 | 0.5 BN | 6555 | Auxiliary Temperature Motor Voltage
3 | 3 BK | 450 | Ground | 3 | 3 BK | 450 | Ground
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 3 RD/BK | 442 | Battery Positive Voltage | 5 | 3 RD/BK | 442 | Battery Positive Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 0.5 OG | 2615 | Auxiliary Mode Door Control (without UK6) | 7 | 0.5 OG | 2615 | Auxiliary Mode Door Control (without UK6)
8 | 0.5 GY | 596 | 5-Volt Reference | 8 | 0.5 GY | 596 | 5-Volt Reference
0.5 GY | 596 | 5-Volt Reference
9 | 0.5 PK | 2145 | Air Temperature Switch Signal - Right | 9 | 0.5 PK | 2145 | Air Temperature Switch Signal - Right
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | 0.5 OG | 2215 | Auxiliary Mode Door Control | 11 | 0.5 OG | 2215 | Auxiliary Mode Door Control
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | 0.5 GY | 2599 | Auxiliary Mode Door Control | 13 | 0.5 GY | 2599 | Auxiliary Mode Door Control
14 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data | 14 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
15 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data | 15 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
16 | 0.5 TN/WH | 372 | Left Audio Signal (-) (U2K or UBS) | 16 | 0.5 TN/WH | 372 | Left Audio Signal (-) (U2K or UBS)
17 | 0.5 BN/WH | 367 | Left Audio Signal (+) (U2K or UBS) | 17 | 0.5 BN/WH | 367 | Left Audio Signal (+) (U2K or UBS)
18 | 0.5 D-GN/WH | 368 | Right Audio Signal (+) (U2K or UBS) | 18 | 0.5 D-GN/WH | 368 | Right Audio Signal (+) (U2K or UBS)
19 | 0.5 GY | 388 | Right Audio Signal (-) (U2K or UBS) | 19 | 0.5 GY | 388 | Right Audio Signal (-) (U2K or UBS)
20 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal | 20 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
21 | 0.5 L-GN/WH | 5729 | Auxiliary Mode Motor Voltage | 21 | 0.5 L-GN/WH | 5729 | Auxiliary Mode Motor Voltage
22 | 0.5 GY | 2614 | Auxiliary Air Temperature Door Control | 22 | 0.5 GY | 2614 | Auxiliary Air Temperature Door Control
23 | 0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control (without UK6) | 23 | 0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control (without UK6)
24 | 0.5 GY/BK | 1798 | Low Reference | 24 | 0.5 GY/BK | 1798 | Low Reference
0.5 GY/BK | 1798 | Low Reference
25 | 0.35 YE | 61 | Low Reference | 25 | 0.35 YE | 61 | Low Reference
26 | 0.8 GY/BK | 690 | Courtesy Lamp High Control | 26 | 0.8 GY/BK | 690 | Courtesy Lamp High Control
27 | 0.5 L-BU | 2088 | Low Reference | 27 | 0.5 L-BU | 2088 | Low Reference
28 | 0.5 D-GN | 2087 | 5-Volt Reference | 28 | 0.5 D-GN | 2087 | 5-Volt Reference
29 | 0.35 WH | 193 | Rear Defog Relay Control | 29 | 0.35 WH | 193 | Rear Defog Relay Control
30 | 0.35 BARE | 6131 | Drain Wire (U2K or UBS) | 30 | 0.35 BARE | 6131 | Drain Wire (U2K or UBS)
31 | 0.5 D-GN | 2211 | Auxiliary Blower Motor Speed Control | 31 | 0.5 D-GN | 2211 | Auxiliary Blower Motor Speed Control
32 | 0.8 BK/WH | 1551 | Ground | 32 | 0.8 BK/WH | 1551 | Ground
33 | 0.35 BARE | 814 | Drain Wire (UE1) | 33 | 0.35 BARE | 814 | Drain Wire (UE1)
34 | 0.35 OG/BK | 1406 | Remote Playback Device Left Audio Signal (UE1) | 34 | 0.35 OG/BK | 1406 | Remote Playback Device Left Audio Signal (UE1)
35 | 0.35 L-BU | 1405 | Remote Playback Device Audio Common Signal (UE1) | 35 | 0.35 L-BU | 1405 | Remote Playback Device Audio Common Signal (UE1)
36 | 0.35 BARE | 6974 | Drain (UVC without U3R or UZR or UVB) | 36 | 0.35 BARE | 6974 | Drain (UVC without U3R or UZR or UVB)
37 | 0.35 PK | 6972 | Camera Signal 2 (+) (UVC without U3R or UZR or UVB) | 37 | 0.35 PK | 6972 | Camera Signal 2 (+) (UVC without U3R or UZR or UVB)
38 | 0.35 L-BU | 6973 | Camera Signal 2 (UVC without U3R or UZR or UVB) | 38 | 0.35 L-BU | 6973 | Camera Signal 2 (UVC without U3R or UZR or UVB)
39 | 0.35 BN/WH | 1571 | Traction Control Switch Signal | 39 | 0.35 BN/WH | 1571 | Traction Control Switch Signal
40 | 0.35 PK | 5149 | Voice Recognition Audio Signal (UE1 with U3R or UZR) | 40 | 0.35 PK | 5149 | Voice Recognition Audio Signal (UE1 with UZR or U3R)
41 | 0.35 PK/BK | 5152 | Low Reference (UE1 with U3R or UZR) | 41 | 0.35 PK/BK | 5152 | Low Reference (UE1 with UZR or U3R)
42 | 0.35 BARE | 1792 | Drain Wire (UE1 with U3R or UZR) | 42 | 0.35 BARE | 1792 | Drain Wire (UE1 with UZR or U3R)
43 | 0.5 YE | 2214 | Auxiliary Air Temperature Door Control (without UK6) | 43 | 0.5 YE | 2214 | Auxiliary Air Temperature Door Control (without UK6)

### X203 Body Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: 7283-3585-40
- Service: See Catalog
- Description: 16-Way F Kaizen YESC Series, Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-5536-40
- Service: See Catalog
- Description: 16-Way M YESC/USCAR Class 3 (L-GY)

#### Terminal Part Information

- Pins: 1-12, 15-16
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 5-8, 13-14
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: Pins: 5-8, 13-14 : E/A
- Core/Insulation Crimp: Pins: 7-8 : See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 8
- Terminal/Tray: 7116-4781-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1-2, 5-6, 13-14
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: Pins: 1-2, 5-6 : E/A
- Core/Insulation Crimp: Pins: 5-6, 13-14 : C/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 3-9, 13-16
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1-2
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X203 Body Harness to Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus- | 1 | 0.8 TN | 2501 | High Speed GMLAN Serial Data Bus-
0.8 TN | 2501 | High Speed GMLAN Serial Data Bus-
2 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 2 | 0.8 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
0.8 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
3 | 0.35 L-BU | 5986 | Communication Enable (MH6) | 3 | 0.35 L-BU | 5986 | Communication Enable (MH6)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.8 BN | 199 | Left Rear Speaker Output (+) (UQA or UQS) | 5 | 0.8 BN | 199 | Left Rear Speaker Output (+) (UQA or UQS)
0.5 BN | 199 | Left Rear Speaker Output (+) (UQF) | 0.5 BN | 199 | Left Rear Speaker Output (+) (UQF)
6 | 0.8 YE | 116 | Left Rear Speaker Output (-) (UQA or UQS) | 6 | 0.8 YE | 116 | Left Rear Speaker Output (-) (UQA or UQS)
0.5 YE | 116 | Left Rear Speaker Output (-) (UQF) | 0.5 YE | 116 | Left Rear Speaker Output (-) (UQF)
7 | 0.5 WH | 1959 | Left Rear Midrange Speaker Output (-) (UQA or UQS) | 7 | 0.8 WH | 1959 | Left Rear Midrange Speaker Output (-) (UQA or UQS)
0.8 WH | 1959 | Left Rear Midrange Speaker Output (-) (UQA or UQS)
8 | 0.8 TN | 1859 | Left Rear Midrange Speaker Output (+) (UQA or UQS) | 8 | 0.8 TN | 1859 | Left Rear Midrange Speaker Output (+) (UQA or UQS)
0.5 TN | 1859 | Left Rear Midrange Speaker Output (+) (UQA or UQS)
9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE) | 9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE)
10 | 0.5 PU | 5357 | Right Tail Lamp Outage Detection Signal (Z88) | 10 | 0.5 PU | 5357 | Right Tail Lamp Outage Detection Signal (Z88)
11 | 0.35 L-GN | 1011 | Remote Radio Control Signal (RCA) | 11 | 0.35 L-GN | 1011 | Remote Radio Control Signal (RCA)
12 | 0.35 PU | 1375 | 12-Volt Reference (RCA) | 12 | 0.35 PU | 1375 | 12-Volt Reference (RCA)
13 | 1 TN | 201 | Left Front Speaker Output (+) | 13 | 1 TN | 201 | Left Front Speaker Output (+)
14 | 1 GY | 118 | Left Front Speaker Output (-) | 14 | 1 GY | 118 | Left Front Speaker Output (-)
15 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | 15 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
16 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal | 16 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal

### X205 Body Harness to Instrument Panel Harness (N38)

#### Connector Part Information

- OEM: 7283-6453-60
- Service: See Catalog
- Description: 16-Way F Kaizen YESC Series, Unsealed (GN)

#### Connector Part Information

- OEM: 7282-6453-60
- Service: See Catalog
- Description: 16-Way M Kaizen YESC Series, Unsealed (GN)

#### Terminal Part Information

- Pins: 7-8
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 5-6
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 2, 4, 9-12
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 3
- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X205 Body Harness to Instrument Panel Harness (N38)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 PK | 2111 | Steering Column Tilt Motor Control - Up | 1 | 1 PK | 2111 | Steering Column Tilt Motor Control - Up
2 | 0.35 OG | 2154 | Steering Column Tilt Sensor Signal | 2 | 0.35 OG | 2154 | Steering Column Tilt Sensor Signal
3 | 1 BN | 2112 | Steering Column Tilt Motor Control - Down | 3 | 1 BN | 2112 | Steering Column Tilt Motor Control - Down
4 | 0.35 OG | 2153 | Steering Column Telescope Sensor Signal | 4 | 0.35 OG | 2153 | Steering Column Telescope Sensor Signal
5 | 1 OG | 2098 | Steering Column Telescope Motor Forward | 5 | 1 OG | 2098 | Steering Column Telescope Motor Forward
6 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38) | 6 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38)
7 | 0.35 TN | 6207 | 5-Volt Reference | 7 | 0.35 TN | 6207 | 5-Volt Reference
8 | 0.35 GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal | 8 | 0.35 GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal
9 | 0.35 GY | 6206 | Low Reference | 9 | 0.35 GY | 6206 | Low Reference
10 | 0.35 OG | 2095 | Steering Column Tilt and Telescope Reverse Switch Signal | 10 | 0.35 OG | 2095 | Steering Column Tilt and Telescope Reverse Switch Signal
11 | 0.35 PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal | 11 | 0.35 PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal
12 | 0.35 YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal | 12 | 0.35 YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal
13-16 | -- | -- | Not Used | 13-16 | -- | -- | Not Used

### X209 Body Harness to Trailer Brake Harness (V92)

#### Connector Part Information

- OEM: 7283-3740-40
- Service: See Catalog
- Description: 6-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-5604-40
- Service: See Catalog
- Description: 6-Way M 6.3 YESC Series (L-GY)

#### Terminal Part Information

- Pins: 2-3
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 1, 5-6
- Terminal/Tray: 7116-4121-02/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Pins: 2-3
- Terminal/Tray: 7114-4120-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 1, 5-6
- Terminal/Tray: 7114-4121-02/9
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### X209 Body Harness to Trailer Brake Harness (V92)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 BK | 550 | Ground | 1 | 2 BK | 550 | Ground
2 | 0.5 GY | 8 | Instrument Panel Lamp Voltage | 2 | 0.5 GY | 8 | Instrument Panel Lamp Voltage
3 | 0.5 WH | 17 | Stop Lamp Voltage | 3 | 0.5 WH | 17 | Stop Lamp Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 2 D-BU | 47 | Trailer Auxiliary Voltage | 5 | 2 D-BU | 47 | Trailer Auxiliary Voltage
6 | 2 RD/BK | 1042 | Battery Positive Voltage | 6 | 2 RD/BK | 1042 | Battery Positive Voltage

### X211 Body Harness to Steering Column Harness

#### Connector Part Information

- OEM: SNAPB-05UN-1FYS
- Service: 13153434
- Description: 5-Way F 0.64 Series Unsealed (YE)

#### Connector Part Information

- OEM: SNAMB-05UN-1FYS
- Service: 19153435
- Description: 5-Way M 0.64 Series Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: SAIT-A03T-M064/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215A/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: SAITW-A03T-064/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-215A(PU)/J-35616-65B (L-BU)

#### X211 Body Harness to Steering Column Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 TN | 3021 | Steering Wheel Module - Stage1 - High Control | 1 | 0.35 TN | 3021 | Steering Wheel Module - Stage1 - High Control
2 | 0.35 BN | 3020 | Steering Wheel Module - Stage1 - Low Control | 2 | 0.35 BN | 3020 | Steering Wheel Module - Stage1 - Low Control
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.35 WH | 3023 | Steering Wheel Module - Stage2 - High Control | 4 | 0.35 WH | 3023 | Steering Wheel Module - Stage2 - High Control
5 | 0.35 PK | 3022 | Steering Wheel Module - Stage2 - Low Control | 5 | 0.35 PK | 3022 | Steering Wheel Module - Stage2 - Low Control

### X214 Instrument Panel Harness to HVAC Harness

#### Connector Part Information

- OEM: 7283-6458-40
- Service: 88988507
- Description: 2-Way F Receptacle 6.3 Series (L-GY)

#### Connector Part Information

- OEM: 7282-6458-40
- Service: See Catalog
- Description: 2-Way M Receptacle 6.3 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X214 Instrument Panel Harness to HVAC Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 3 RD/BK | 442 | Battery Positive Voltage | 1 | 3 RD/BK | 442 | Battery Positive Voltage
2 | 3 BK | 450 | Ground | 2 | 3 BK | 450 | Ground

### X216 Instrument Panel Harness to Headliner Harness (U42)

#### Connector Part Information

- OEM: 7283-6388-40
- Service: See Catalog
- Description: 20-Way F Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-6568-40
- Service: See Catalog
- Description: 20-Way M YESC Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: 7114-4720-02/14
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### X216 Instrument Panel Harness to Headliner Harness (U42)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 BARE | 6980 | DVD Audio Shield | 1 | 0.35 BARE | 6980 | DVD Audio Shield
2 | 0.35 L-BU | 5826 | Left DVD Audio Signal (+) | 2 | 0.35 L-BU | 5826 | Left DVD Audio Signal (+)
3 | 0.35 PU | 6979 | DVD Audio Common | 3 | 0.35 PU | 6979 | DVD Audio Common
4 | 0.35 WH | 5828 | Right DVD Audio Signal (+) | 4 | 0.35 WH | 5828 | Right DVD Audio Signal (+)
5 | 0.35 TN/WH | 5830 | Remote Infra Red Signal (-) | 5 | 0.35 TN/WH | 5830 | Remote Infra Red Signal (-)
6 | 0.35 OG/BK | 5831 | Remote Infra Red Signal (+) | 6 | 0.35 OG/BK | 5831 | Remote Infra Red Signal (+)
7 | 0.35 BN/WH | 5331 | Low Reference | 7 | 0.35 BN/WH | 5331 | Low Reference
8 | 0.35 PU/WH | 5330 | Right Infra Red Audio Signal | 8 | 0.35 PU/WH | 5330 | Right Infra Red Audio Signal
9 | 0.35 OG/BK | 5329 | Left Rear Low Level Audio Signal (+) | 9 | 0.35 OG/BK | 5329 | Left Rear Low Level Audio Signal (+)
10 | 0.35 BARE | 5332 | Infra Red Audio Drain Wire | 10 | 0.35 BARE | 5332 | Infra Red Audio Drain Wire
11 | 0.35 WH/BK | 5335 | DVD Video Signal (-) | 11 | 0.35 WH/BK | 5335 | DVD Video Signal (-)
12 | 0.35 D-GN | 6975 | DVD Video Signal (+) | 12 | 0.35 D-GN | 6975 | DVD Video Signal (+)
13 | 0.35 BARE | 6976 | DVD Video Drain Wire | 13 | 0.35 BARE | 6976 | DVD Video Drain Wire
14 | 0.35 WH | 7066 | Entertainment Remote Enable Signal | 14 | 0.35 WH | 7066 | Entertainment Remote Enable Signal
15 | 0.35 L-GN/BK | 5845 | Video Module Signal | 15 | 0.35 L-GN/BK | 5845 | Video Module Signal
16 | 0.35 PK/BK | 5844 | Video Bright Control | 16 | 0.35 PK/BK | 5844 | Video Bright Control
17-20 | -- | -- | Not Used | 17-20 | -- | -- | Not Used

### X240 Instrument Panel Harness to Floor Console Harness

#### Connector Part Information

- OEM: 7283-6537-30
- Service: See Catalog
- Description: 26-Way F YESC LIF Series (BK)

#### Connector Part Information

- OEM: 7282-6537-30
- Service: See Catalog
- Description: 26-Way M YESC LIF Series (BK)

#### Terminal Part Information

- Pins: 17, 26
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 2-25
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 17
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 17, 26
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 18-20
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 2-25
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X240 Instrument Panel Harness to Floor Console Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 GY | 391 | Rear Window Wiper Switch Signal | 1 | 0.5 GY | 391 | Rear Window Wiper Switch Signal
2 | 0.35 PU/WH | 5330 | Right Infra Red Audio Signal (U42) | 2 | 0.35 PU/WH | 5330 | Right Infra Red Audio Signal (U42)
3 | 0.35 BN/WH | 5331 | Low Reference (U42) | 3 | 0.35 BN/WH | 5331 | Low Reference (U42)
4 | 0.35 BARE | 5332 | Infra Red Audio Drain Wire (U42) | 4 | 0.35 BARE | 5332 | Infra Red Audio Drain Wire (U42)
5 | 0.35 OG/BK | 5329 | Left Rear Low Level Audio Signal (+) (U42) | 5 | 0.35 OG/BK | 5329 | Left Rear Low Level Audio Signal (+) (U42)
6 | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control | 6 | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control
7 | 0.35 L-BU | 553 | Tow/Haul Switch Signal | 7 | 0.35 L-BU | 553 | Tow/Haul Switch Signal
8 | 0.5 L-GN | 2270 | Rear Window Washer Relay Control | 8 | 0.5 L-GN | 2270 | Rear Window Washer Relay Control (W49)
9 | 0.35 BARE | 5345 | Drain Wire (U42) | 9 | 0.35 BARE | 5345 | Drain Wire (U42)
10 | 0.35 WH | 2058 | Auxiliary Audio Right Signal (U42) | 10 | 0.35 WH | 2058 | Auxiliary Audio Right Signal (U42)
11 | 0.35 YE | 2059 | Auxiliary Audio Left Signal (U42) | 11 | 0.35 YE | 2059 | Auxiliary Audio Left Signal (U42)
12 | 0.35 PU | 5526 | Memory Set Switch Signal | 12 | 0.35 PU | 5526 | Memory Set Switch Signal
13 | 0.35 BARE | 5346 | Drain Wire (U42) | 13 | 0.35 BARE | 5346 | Drain Wire (U42)
14 | 0.35 PU | 2056 | Auxiliary Video High Signal (U42) | 14 | 0.35 PU | 2056 | Auxiliary Video High Signal (U42)
15 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Voltage | 15 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Voltage
16 | 0.35 PU | 1375 | 12-Volt Reference | 16 | 0.35 PU | 1375 | 12-Volt Reference
17 | 0.35 L-BU | 5312 | RSA Left Audio Signal (UK6) | 17 | 0.8 L-BU | 5312 | RSA Left Audio Signal (UK6)
18 | 0.35 BN | 5314 | RSA Audio Common Signal (UK6) | 18 | 0.8 BN | 5314 | RSA Audio Common Signal (UK6)
19 | 0.35 L-GN | 5313 | RSA Right Audio Signal (UK6) | 19 | 0.8 L-GN | 5313 | RSA Right Audio Signal (UK6)
20 | 0.35 TN/WH | 5830 | Remote Infra Red Signal (-) (UK6) | 20 | 0.8 TN/WH | 5830 | Remote Infra Red Signal (-) (UK6)
21 | 0.35 BARE | 6759 | Discrete Audio Drain Wire (UK6 without UQF) | 21 | 0.35 BARE | 6759 | Discrete Audio Drain Wire (UK6 without UQF)
22 | 0.35 D-BU | 546 | Right Rear Low Level Audio Signal (+) (UK6) | 22 | 0.8 D-BU | 546 | Right Rear Low Level Audio Signal (+) (UK6)
23 | 0.35 TN | 1946 | Right Rear Low Level Audio Signal (-) (UK6) | 23 | 0.8 TN | 1946 | Right Rear Low Level Audio Signal (-) (UK6)
24 | 0.35 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (UK6) | 24 | 0.8 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (UK6)
25 | 0.35 BN | 1999 | Left Rear Low Level Audio Signal (-) (UK6) | 25 | 0.8 BN | 1999 | Left Rear Low Level Audio Signal (-) (UK6)
26 | 0.35 BARE | 1574 | Drain Wire (UK6 without UQF) | 26 | 0.35 BARE | 1574 | Drain Wire (UK6 without UQF)

### X252 Body Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: GT13-1/1PP-HU
- Service: See Catalog
- Description: 3-Way F GT13 Coaxial Series (WH)

#### Connector Part Information

- OEM: GT13GM-1/1S-HU
- Service: See Catalog
- Description: 3-Way M GT13 Coaxial Series (WH)

#### Terminal Part Information

- Terminal/Tray: 7114-4618-02/27
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-65B (L-BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X252 Body Harness to Instrument Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 WH | 7066 | Entertainment Remote Enable Signal | 1 | 0.35 WH | 7066 | Entertainment Remote Enable Signal
C | -- | -- | Coax | C | -- | -- | Coax
S | -- | -- | Not Used | S | -- | -- | Not Used

### X305 Fuel Tank Harness to Body Harness

#### Connector Part Information

- OEM: 12176335
- Service: 15305944
- Description: 8-Way F Metri-Pack Mixed Series, Sealed (WH)

#### Connector Part Information

- OEM: 13609624
- Service: See Catalog
- Description: 16-Way M Metri-Pack Mixed Series, Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 3A, 3C
- Terminal/Tray: 12129497/1
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 3B, 3D, 3E, 3F, 3H, 3G
- Terminal/Tray: 12048159/2
- Core/Insulation Crimp: Pins: 3B, 3D, 3E, 3F, 3H : See Terminal Repair Kit
- Core/Insulation Crimp: Pins: 3G : 2/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X305 Fuel Tank Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
-- | -- | -- | Not Used | 1A-1D | -- | -- | Not Used
-- | -- | -- | Not Used | 2A-2D | -- | -- | Not Used
A | -- | -- | Not Used | 3A | -- | -- | Not Used
B | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal | 3B | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
C | -- | -- | Not Used | 3C | -- | -- | Not Used
D | 0.35 L-BU/WH | 1589 | Fuel Level Sensor Signal | 3D | 0.35 PU | 1589 | Fuel Level Sensor Signal
E | 0.35 TN | 452 | Low Reference | 3E | 0.35 TN | 452 | Low Reference
F | 0.35 WH | 1310 | EVAP Canister Vent Solenoid Control | 3F | 0.35 WH | 1310 | EVAP Canister Vent Solenoid Control
G | 0.5 RD/WH | 4140 | Battery Positive Voltage | 3G | 0.5 RD/WH | 4140 | Battery Positive Voltage
H | 0.35 GY | 2709 | 5-Volt Reference | 3H | 0.35 GY | 2709 | 5-Volt Reference

### X308 Rear Chassis Harness to Fuel Tank Harness

#### Connector Part Information

- OEM: 7283-5577-10
- Service: 88988393
- Description: 6-Way F YESC/USCAR Class III Series (D-GY)

#### Connector Part Information

- OEM: 7282-5577-10
- Service: See Catalog
- Description: 6-Way M YESC/USCAR Class III Series (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X308 Rear Chassis Harness to Fuel Tank Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 GY | 120 | Fuel Pump Voltage | 1 | 2 GY | 120 | Fuel Pump Voltage
2 | 2 PK | 1850 | Ground | 2 | 2 PK | 1850 | Ground
3 | 0.5 GY | 7443 | Drain Wire | 3 | 0.5 GY | 7443 | Drain Wire
4 | 0.35 BN | 7445 | 5-Volt Reference | 4 | 0.35 BN | 7445 | 5-Volt Reference
5 | 0.35 PU | 7446 | Fuel Pressure Sensor Signal | 5 | 0.35 PU | 7446 | Fuel Pressure Sensor Signal
6 | 0.35 GY | 7447 | Low Reference | 6 | 0.35 GY | 7447 | Low Reference

### X314 Body Harness to Passenger Seat Harness

#### Connector Part Information

- OEM: 7283-6376-30
- Service: See Catalog
- Description: 26-Way F Hybrid (BK)

#### Connector Part Information

- OEM: 7282-6376-30
- Service: See Catalog
- Description: 26-Way M Hybrid (BK)

#### Terminal Part Information

- Pins: 3, 5-6, 9-10, 13, 19, 21
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 2, 12, 23
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: Pins: 12 : E/A
- Core/Insulation Crimp: Pins: 2, 23 : See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 17, 26
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 8
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Pins: 12, 17, 26
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 2, 5-6, 9-10, 13, 19, 21, 23
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1, 8
- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### X314 Body Harness to Passenger Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 3 BK | 750 | Ground (AG2 or AAQ or KB6) | 1 | 3 BK | 750 | Ground (AG2 or AAQ or KB6)
2 | 0.35 BK/WH | 1751 | Ground | 2 | 0.35 BK/WH | 1751 | Ground
0.5 BK/WH | 1751 | Ground
3-4 | -- | -- | Not Used | 3-4 | -- | -- | Not Used
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | 5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6 | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal | 6 | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | 3 RD/WH | 3040 | Battery Positive Voltage (AG2 or AAQ) | 8 | 3 RD/WH | 3040 | Battery Positive Voltage (AG2 or AAQ)
9 | 0.35 L-BU | 5476 | Low Reference (KA1 or KB6) | 9 | 0.35 L-BU | 5476 | Low Reference (KA1 or KB6)
10 | 0.35 RD/WH | 1340 | Battery Positive Voltage | 10 | 0.35 RD/WH | 1340 | Battery Positive Voltage
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | 0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control (KA1 or KB6) | 12 | 0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control (KA1 or KB6)
13 | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal (KA1 or KB6) | 13 | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal (KA1 or KB6)
14-16 | -- | -- | Not Used | 14-16 | -- | -- | Not Used
17 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control (KA1) | 17 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control (KA1)
2 RD/WH | 640 | Battery Positive Voltage (KB6) | 2 RD/WH | 640 | Battery Positive Voltage (KB6)
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal (KA1) | 19 | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal (KA1)
20 | 0.35 GY | 5961 | Right Heated/Cooled Seat Mode Signal (KB6) | 20 | 0.35 GY | 5961 | Right Heated/Cooled Seat Mode Signal (KB6)
21 | 0.35 TN | 2482 | Low Reference (KA1) | 21 | 0.35 TN | 2482 | Low Reference (KA1)
22 | -- | -- | Not Used | 22 | -- | -- | Not Used
23 | 0.35 PK | 5057 | Low Reference | 23 | 0.35 PK | 5057 | Low Reference
0.35 PK | 5057 | Low Reference
24-25 | -- | -- | Not Used | 24-25 | -- | -- | Not Used
26 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage (KA1 or KB6) | 26 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage (KA1 or KB6)

### X315 Body Harness to Driver Seat Harness

#### Connector Part Information

- OEM: 7283-4190-30
- Service: See Catalog
- Description: 43-Way F YESC Unsealed Series (BK)

#### Connector Part Information

- OEM: 7282-4190-30
- Service: See Catalog
- Description: 43-Way M YESC Unsealed Series (BK)

#### Terminal Part Information

- Pins: 8-22, 24-31, 33, 35, 37-42
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 1, 7, 23, 32, 34, 36,
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 2, 43
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: Pins: 43 : C/A
- Core/Insulation Crimp: Pins: 2 : E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 3, 5
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 43
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 1-2, 7, 32
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: Pins: 2 : E/A
- Core/Insulation Crimp: Pins: 1, 7, 32 : C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 16, 22-24, 26, 28-29, 34, 36
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: Pins: 23, 36 : E/A
- Core/Insulation Crimp: Pins: 34 : C/A
- Core/Insulation Crimp: Pins: 16, 22, 24, 26, 28-29 : See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 9-11, 13-15, 17, 21, 25, 27
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 3, 5
- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 43
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X315 Body Harness to Driver Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 OG | 2098 | Steering Column Telescope Motor Forward (N38) | 1 | 1 OG | 2098 | Steering Column Telescope Motor Forward (N38)
2 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control (KA1) | 2 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control (KA1)
3 | 3 RD/WH | 1140 | Battery Positive Voltage (AG1 or AG3 or AH5 or A45) | 3 | 3 RD/WH | 1140 | Battery Positive Voltage (AG1 or AG3 or AH5 or A45)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 3 BK | 550 | Ground (AG1 or AG3 or AH5 or A45 or KA1 or KB6) | 5 | 3 BK | 550 | Ground (AG1 or AG3 or AH5 or A45 or KA1 or KB6)
6 | 2 RD/WH | 640 | Battery Positive Voltage (KA1 without A45) | 6 | 2 RD/WH | 640 | Battery Positive Voltage (KA1 without A45)
2 RD/WH | 640 | Battery Positive Voltage (KB6) | 2 RD/WH | 640 | Battery Positive Voltage (KB6)
7 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38) | 7 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38)
8 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (KA1 without A45) | 8 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (KA1 without A45)
9 | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal (KA1 or KB6) | 9 | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal (KA1 or KB6)
10 | 0.35 RD/WH | 3140 | Battery Positive Voltage (A45) | 10 | 0.35 RD/WH | 3140 | Battery Positive Voltage (A45)
11 | 0.35 D-GN | 5016 | Seat Belt Switch - Left - Signal | 11 | 0.35 D-GN | 5016 | Seat Belt Switch - Left - Signal
12 | -- | -- | Not Used | 12 | -- | -- | Not Used
13 | 0.35 L-BU | 5476 | Low Reference (KA1 or KB6) | 13 | 0.35 L-BU | 5476 | Low Reference (KA1 or KB6)
14 | 0.35 PK | 5057 | Low Reference | 14 | 0.35 PK | 5057 | Low Reference
15 | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal (KA1) | 15 | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal (KA1)
16 | 0.35 GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal (N38) | 16 | 0.35 GY | 2096 | Steering Column Tilt and Telescope Up Switch Signal (N38)
17 | 0.35 TN | 2482 | Low Reference (KA1) | 17 | 0.35 TN | 2482 | Low Reference (KA1)
18 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (KA1 without A45) | 18 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (KA1 without A45)
19 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (KA1 without A45) | 19 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (KA1 without A45)
20 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (KA1 without A45) | 20 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (KA1 without A45)
21 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (A45 or KA1) | 21 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (A45 or KA1)
22 | 0.35 OG | 2153 | Steering Column Telescope Sensor Signal (N38) | 22 | 0.35 OG | 2153 | Steering Column Telescope Sensor Signal (N38)
23 | 0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control (KA1 or KB6) | 23 | 0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control (KA1 or KB6)
24 | 0.35 YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal (N38) | 24 | 0.35 YE | 2097 | Steering Column Tilt and Telescope Down Switch Signal (N38)
25 | 0.35 GY | 6206 | Low Reference (N38) | 25 | 0.35 GY | 6206 | Low Reference (N38)
26 | 0.35 PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal (N38) | 26 | 0.35 PK | 2094 | Steering Column Tilt and Telescope Forward Switch Signal (N38)
27 | 0.35 TN | 6207 | 5-Volt Reference (N38) | 27 | 0.35 TN | 6207 | 5-Volt Reference (N38)
28 | 0.35 OG | 2095 | Steering Column Tilt and Telescope Reverse Switch Signal (N38) | 28 | 0.35 OG | 2095 | Steering Column Tilt and Telescope Reverse Switch Signal (N38)
29 | 0.35 OG | 2154 | Steering Column Tilt Sensor Signal (N38) | 29 | 0.35 OG | 2154 | Steering Column Tilt Sensor Signal (N38)
30 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (KA1 without A45) | 30 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (KA1 without A45)
31 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (KA1 without A45) | 31 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (KA1 without A45)
32 | 1 PK | 2111 | Steering Column Tilt Motor Control - Up (N38) | 32 | 1 PK | 2111 | Steering Column Tilt Motor Control - Up (N38)
33 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (KA1 without A45) | 33 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (KA1 without A45)
34 | 1 BN | 2112 | Steering Column Tilt Motor Control - Down (N38) | 34 | 1 BN | 2112 | Steering Column Tilt Motor Control - Down (N38)
35 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (KA1 without A45) | 35 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (KA1 without A45)
36 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage (KA1 or KB6) | 36 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage (KA1 or KB6)
37 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (KA1 without A45) | 37 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (KA1 without A45)
38 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (KA1 without A45) | 38 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (KA1 without A45)
39 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (KA1 without A45) | 39 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (KA1 without A45)
0.35 GY | 5961 | Right Heated/Cooled Seat Mode Signal (KB6) | 0.35 GY | 5961 | Right Heated/Cooled Seat Mode Signal (KB6)
40 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (KA1 without A45) | 40 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (KA1 without A45)
41 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (KA1 without A45) | 41 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (KA1 without A45)
42 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (KA1 without A45) | 42 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (KA1 without A45)
43 | 2 RD/WH | 4040 | Battery Positive Voltage (N38) | 43 | 2 RD/WH | 4040 | Battery Positive Voltage (N38)

### X320 Headliner Harness to Body Harness (DNP or UD7 or UE1)

#### Connector Part Information

- OEM: 7283-6388-40
- Service: See Catalog
- Description: 20-Way F Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-6568-40
- Service: See Catalog
- Description: 20-Way M YESC Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: Pins: 1-6, 10, 15-16 : H/H
- Core/Insulation Crimp: Pins: 7-9 : J/J
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: 7114-4720-02/14
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### X320 Headliner Harness to Body Harness (DNP or UD7 or UE1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP) | 1 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP)
2 | 0.35 BK/RD | 1691 | Low Reference (DNP) | 2 | 0.35 PK | 1691 | Low Reference (DNP)
3 | 0.35 WH | 2370 | Telltale Assembly Voltage (UD7) | 3 | 0.35 WH | 2370 | Telltale Assembly Voltage (UD7)
4 | 0.35 OG | 2371 | Left Amber Indicator Control (UD7) | 4 | 0.35 OG | 2371 | Left Amber Indicator Control (UD7)
5 | 0.35 D-BU | 2372 | Center Amber Indicator Control (UD7) | 5 | 0.35 D-BU | 2372 | Center Amber Indicator Control (UD7)
6 | 0.35 GY | 2373 | Red Indicator Control (UD7) | 6 | 0.35 GY | 2373 | Red Indicator Control (UD7)
7 | 0.5 BK/GN | 2514 | Keypad Signal (UE1) | 7 | 0.35 D-GN/WH | 2514 | Keypad Signal (UE1)
8 | 0.5 BK/L-GN | 2515 | Keypad Voltage (UE1) | 8 | 0.35 L-GN/BK | 2515 | Keypad Voltage (UE1)
9 | 0.5 BK/GY | 2516 | Keypad Green LED Signal (UE1) | 9 | 0.35 YE/BK | 2516 | Keypad Green LED Signal (UE1)
10 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1) | 10 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1)
11 | 0.35 OG | 300 | Power Mode | 11 | 0.35 OG | 300 | Power Mode
12 | 0.35 GY | 6135 | Local Interconnect Network (LIN) (U80) | 12 | 0.35 GY | 6135 | Local Interconnect Network (LIN) (U80)
13-14 | -- | -- | Not Used | 13-14 | -- | -- | Not Used
15 | 0.35 BARE | 514 | Ground (UE1) | 15 | 0.35 BARE | 514 | Ground (UE1)
16 | 0.35 GY | 655 | Cellular Microphone Signal (UE1) | 16 | 0.35 GY | 655 | Cellular Microphone Signal (UE1)
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | 0.35 BARE | 6974 | Drain Wire (UVC without U3R or UZR or UVB) | 18 | 0.35 BARE | 6974 | Drain Wire (UVC without U3R or UZR or UVB)
19 | 0.35 PK | 6972 | Camera Video Signal (+) (UVC without U3R or UZR or UVB) | 19 | 0.35 PK | 6972 | Camera Video Signal (+) (UVC without U3R or UZR or UVB)
20 | 0.35 L-BU | 6973 | Camera Video Signal (-) (UVC without U3R or UZR or UVB) | 20 | 0.35 L-BU | 6973 | Camera Video Signal (-) (UVC without U3R or UZR or UVB)

### X322 Body Harness to Headliner Harness

#### Connector Part Information

- OEM: 7283-6447-40
- Service: 88956523
- Description: 14-Way F Hybrid Series (L-GY)

#### Connector Part Information

- OEM: 7282-6447-40
- Service: 88956523
- Description: 14-Way M Hybrid Series (L-GY)

#### Terminal Part Information

- Pins: 2-3, 5, 9-12
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 7-8
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: Pins: 8 : E/A
- Core/Insulation Crimp: Pins: 7 : See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 14
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 8
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 7
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 4
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 2-3, 5, 9-12
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1, 14
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X322 Body Harness to Headliner Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 3 RD/WH | 3440 | Battery Positive Voltage (C3U) | 1 | 3 RD/WH | 3440 | Battery Positive Voltage (C3U)
2 | 0.5 BK/WH | 38 | Backup Lamp Voltage (DD8) | 2 | 0.5 D-BU | 38 | Backup Lamp Voltage (DD8)
3 | 0.35 BK/YE | 43 | Ignition Voltage (DD8) | 3 | 0.35 YE | 43 | Ignition Voltage (C3U or DD8)
0.35 YE | 43 | Ignition Voltage (C3U)
4 | 0.8 OG | 1732 | Courtesy Lamps Voltage | 4 | 0.8 OG | 1732 | Courtesy Lamps Voltage
5 | 0.5 PK | 5829 | Infra Red Module Voltage (U42) | 5 | 0.35 PK | 5829 | Infra Red Module Voltage (U42)
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 0.5 BK/WH | 351 | Ground (U42) | 7 | 0.5 BK/WH | 351 | Ground (U42)
0.5 BK/WH | 351 | Ground (U42)
8 | 0.8 GY/BK | 690 | Courtesy Lamp High Control | 8 | 0.8 GY/BK | 690 | Courtesy Lamp High Control
9 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (UG1 or C3U) | 9 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (UG1 or C3U)
10 | 0.5 RD/WH | 2340 | Battery Positive Voltage (U42) | 10 | 0.5 RD/WH | 2340 | Battery Positive Voltage (U42)
11 | 0.35 RD/WH | 3140 | Battery Positive Voltage (UG1) | 11 | 0.35 RD/WH | 3140 | Battery Positive Voltage (UG1)
12 | 0.35 PU/WH | 1382 | LED Dimming Signal | 12 | 0.35 PU/WH | 1382 | LED Dimming Signal
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | 3 BK | 850 | Ground | 14 | 3 BK | 850 | Ground

### X324 Battery Negative Cable Harness to Body Harness

#### Connector Part Information

- OEM: 7283-6443-40
- Service: See Catalog
- Description: 2-Way F 1.5 YESC Series, Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-6443-40
- Service: See Catalog
- Description: 2-Way M 1.5 Series, Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X324 Battery Negative Cable Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BK | 50 | Ground | 1 | 0.35 BK | 50 | Ground
2 | -- | -- | Not Used | 2 | -- | -- | Not Used

### X325 Battery Positive Cable Harness to Body Harness (UE1)

#### Connector Part Information

- OEM: 7283-6444-60
- Service: See Catalog
- Description: 2-Way F 1.5 YESC Series, Unsealed (GN)

#### Connector Part Information

- OEM: 7282-6444-60
- Service: See Catalog
- Description: 2-Way M 1.5 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X325 Battery Positive Cable Harness to Body Harness (UE1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 RD/WH | 4640 | Battery Positive Voltage | 1 | 1 RD | 4640 | Battery Positive Voltage
2 | -- | -- | Not Used | 2 | -- | -- | Not Used

### X332 Body Harness to Passenger Seat SIR Jumper Harness

#### Connector Part Information

- OEM: SNAPB-05UN-1FYS
- Service: 13153434
- Description: 5-Way F 0.64 Series Unsealed (YE)

#### Connector Part Information

- OEM: SNAMB-05UN-1FYS
- Service: 19153435
- Description: 5-Way M 0.64 Series Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: SAIT-A03T-M064/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215A/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: SAITW-A03T-064/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-215A(PU)/J-35616-65B (L-BU)

#### X332 Body Harness to Passenger Seat SIR Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 TN | 3062 | Seat Belt Buckle Pretensioner - Right - High Control | 1 | L-GN/RD | -- | Seat Belt Buckle Pretensioner - Right - High Control
2 | 0.5 L-BU/BK | 3063 | Seat Belt Buckle Pretensioner - Right - Low Control | 2 | WH/RD | -- | Seat Belt Buckle Pretensioner - Right - Low Control
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.5 TN/WH | 2135 | Side Impact Module - Right Front - High Control | 4 | WH/RD | -- | Side Impact Module - Right Front - High Control
5 | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control | 5 | L-GN/RD | -- | Side Impact Module - Right Front - Low Control

### X333 Body Harness to Driver Seat SIR Jumper Harness

#### Connector Part Information

- OEM: SNAPB-05UN-1FYS
- Service: 13153434
- Description: 5-Way F 0.64 Series Unsealed (YE)

#### Connector Part Information

- OEM: SNAMB-05UN-1FYS
- Service: 19153435
- Description: 5-Way M 0.64 Series Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: SAIT-A03T-M064/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215A/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: SAITW-A03T-064/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-215A(PU)/J-35616-65B (L-BU)

#### X333 Body Harness to Driver Seat SIR Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 WH | 3064 | Seat Belt Buckle Pretensioner - Left - High Control | 1 | L-GN/RD | -- | Seat Belt Buckle Pretensioner - Left - High Control
2 | 0.5 YE/BK | 3065 | Seat Belt Buckle Pretensioner - Left - Low Control | 2 | WH/RD | -- | Seat Belt Buckle Pretensioner - Left - Low Control
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control | 4 | WH/RD | -- | Side Impact Module - Left Front - High Control
5 | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control | 5 | L-GN/RD | -- | Side Impact Module - Left Front - Low Control

### X340 Floor Console Harness to Body Harness

#### Connector Part Information

- OEM: 7283-4190-30
- Service: See Catalog
- Description: 43-Way F YESC Unsealed Series (BK)

#### Connector Part Information

- OEM: 7282-4190-30
- Service: See Catalog
- Description: 43-Way M YESC Unsealed Series (BK)

#### Terminal Part Information

- Pins: 1, 32
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 3
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 2, 8-15, 17, 20-22, 24-29, 33-40
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: Pins: 8-15, 17, 20-22, 24-29, 33-40 : E/C
- Core/Insulation Crimp: Pins: 2 : See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 7, 16, 23, 43
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: Pins: 7, 43 : E/A
- Core/Insulation Crimp: Pins: 16, 23 : See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 5
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Pins: 2-3, 7
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: Pins: 2, 7 : E/A
- Core/Insulation Crimp: Pins: 3 : C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1, 8-17, 20-29, 32-40, 42
- Terminal/Tray: 7114-4100-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 5
- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 43
- Terminal/Tray: 7116-4150-02/9
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### X340 Floor Console Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BK/WH | 351 | Ground (UK6) | 1 | 0.5 BK/WH | 351 | Ground (UK6)
2 | 0.8 D-BU | 6807 | 120 VAC Inverter Control (KV1) | 2 | 0.8 D-BU | 6807 | 120 VAC Inverter Control (KV1)
3 | 1 RD/WH | 2540 | Battery Positive Voltage | 3 | 1 RD/WH | 2540 | Battery Positive Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 3 BK | 750 | Ground | 5 | 3 BK | 750 | Ground
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 0.8 RD | 5684 | 120 VAC Phase B (KV1) | 7 | 0.8 RD | 5684 | 120 VAC Phase B (KV1)
8 | 0.5 RD/WH | 2340 | Battery Positive Voltage (UK6) | 8 | 0.5 RD/WH | 2340 | Battery Positive Voltage (UK6)
9 | 0.35 D-GN | 6112 | Power Liftgate On/Off Switch Signal (TB5) | 9 | 0.35 D-GN | 6112 | Power Liftgate On/Off Switch Signal (TB5)
10 | 0.35 GY | 8 | Instrument Panel Lamp Voltage | 10 | 0.35 GY | 8 | Instrument Panel Lamp Voltage
11 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (KA1 or KB6) | 11 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (KA1 or KB6)
12 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (KA1 or KB6) | 12 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (KA1 or KB6)
13 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (KA1 or KB6) | 13 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (KA1 or KB6)
14 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (KA1 or KB6) | 14 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (KA1 or KB6)
15 | 0.35 D-GN/WH | 5800 | Liftgate Open/Close Switch Signal (TB5) | 15 | 0.35 D-GN/WH | 5800 | Liftgate Open/Close Switch Signal (TB5)
16 | 0.35 PU/WH | 6816 | Heated Seat Indicator Dimming (KA1) | 16 | 0.35 PU/WH | 6816 | Heated Seat Indicator Dimming (KA1 without A45)
0.35 PU/WH | 6816 | Heated Seat Indicator Dimming (KA1)
17 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (KA1 or KB6) | 17 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (KA1 or KB6)
18-19 | -- | -- | Not Used | 18-19 | -- | -- | Not Used
20 | 0.35 PU/WH | 1382 | LED Dimming Signal | 20 | 0.35 PU/WH | 1382 | LED Dimming Signal
21 | 0.35 PK | 5829 | Infra Red Module Voltage (U42) | 21 | 0.35 PK | 5829 | Infra Red Module Voltage (U42)
22 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (UK6) | 22 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (UK6)
23 | 0.35 YE | 43 | Ignition Voltage | 23 | 0.35 YE | 43 | Ignition Voltage
0.35 YE | 43 | Ignition Voltage (KV1)
24 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (KA1 or KB6) | 24 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (KA1 or KB6)
25 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (KA1 or KB6) | 25 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (KA1 or KB6)
26 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (KA1 or KB6) | 26 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (KA1 or KB6)
27 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (KA1 or KB6) | 27 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (KA1 or KB6)
28 | 0.35 BN/WH | 1571 | Traction Control Switch Signal | 28 | 0.35 BN/WH | 1571 | Traction Control Switch Signal
29 | 0.5 GY/BK | 1798 | Low Reference (without UK6) | 29 | 0.5 GY/BK | 1798 | Low Reference (without UK6)
30-31 | -- | -- | Not Used | 30-31 | -- | -- | Not Used
32 | 0.5 GY | 596 | 5-Volt Reference (without UK6) | 32 | 0.5 GY | 596 | 5-Volt Reference (without UK6)
33 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (KA1 or KB6) | 33 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (KA1 or KB6)
34 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (KA1 or KB6) | 34 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (KA1 or KB6)
35 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (KA1 or KB6) | 35 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (KA1 or KB6)
36 | 0.5 YE | 2214 | Auxiliary Air Temperature Door Control (without UK6) | 36 | 0.5 YE | 2214 | Auxiliary Air Temperature Door Control (without UK6)
37 | 0.5 OG | 2615 | Auxiliary Mode Door Control (without UK6) | 37 | 0.5 OG | 2615 | Auxiliary Mode Door Control (without UK6)
38 | 0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control (without UK6) | 38 | 0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control (without UK6)
39 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (KA1 or KB6) | 39 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (KA1 or KB6)
40 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (KA1 or KB6) | 40 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (KA1 or KB6)
41 | -- | -- | Not Used | 41 | -- | -- | Not Used
42 | 0.35 WH | 2283 | Rear Wiper/Washer Switch Voltage (W49) | 42 | 0.35 WH | 2283 | Rear Wiper/Washer Switch Voltage (W49)
43 | 0.8 BK | 5683 | 120 VAC Phase A (KV1) | 43 | 0.8 BK | 5683 | 120 VAC Phase A (KV1)

### X341 Floor Console Harness to A/T Shifter Harness

#### Connector Part Information

- OEM: 12047886
- Service: 12101822
- Description: 8-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12045688
- Service: 12101827
- Description: 8-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X341 Floor Console Harness to A/T Shifter Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 YE | 43 | Ignition Voltage | A | 0.35 WH | -- | Ignition Voltage
B | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control | B | 0.35 WH | -- | Steering Column Key Cylinder Lock Solenoid Control
C | 0.35 GY | 8 | Instrument Panel Lamp Voltage | C | 0.35 BU | -- | Instrument Panel Lamp Voltage
D | 0.35 BK | 750 | Ground | D | 0.35 BU | -- | Ground
E | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Voltage | E | 0.35 BK | -- | A/T Shift Lock Control Solenoid Voltage
F | 0.35 BK | 750 | Ground | F | 0.35 BK | -- | Ground
G | 0.35 PU | 1375 | 12-Volt Reference | G | 0.35 GN | -- | 12-Volt Reference
H | 0.35 PU | 5526 | Shift Request Switch Signal | H | 0.35 GN | -- | Shift Request Switch Signal

### X343 Headliner Harness to Overhead Console Harness

#### Connector Part Information

- OEM: 7283-6453-60
- Service: See Catalog
- Description: 16-Way F Kaizen YESC Series, Unsealed (GN)

#### Connector Part Information

- OEM: 7282-6453-60
- Service: See Catalog
- Description: 16-Way M Kaizen YESC Series (GN)

#### Terminal Part Information

- Pins: 1, 6-7, 9-10, 13, 16
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 8
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1, 13
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 2-3, 7-10, 14-16
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 6
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### X343 Headliner Harness to Overhead Console Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 OG | 1732 | Courtesy Lamps Voltage | 1 | 0.8 OG | 1732 | Courtesy Lamps Voltage
2 | 0.35 BN | 100 | Sunroof Switch Open Signal (C3U) | 2 | 0.35 BN | 100 | Sunroof Switch Open Signal (C3U)
3 | 0.35 OG | 110 | Sunroof Switch Close Signal (C3U) | 3 | 0.35 OG | 110 | Sunroof Switch Close Signal (C3U)
4-5 | -- | -- | Not Used | 4-5 | -- | -- | Not Used
6 | 0.35 RD/WH | 3140 | Battery Positive Voltage (UG1) | 6 | 0.5 RD/WH | 3140 | Battery Positive Voltage (UG1)
7 | 0.35 PU/WH | 1382 | LED Dimming Signal | 7 | 0.35 PU/WH | 1382 | LED Dimming Signal
8 | 0.5 BK | 850 | Ground | 8 | 0.5 BK | 850 | Ground
0.5 BK | 850 | Ground (DH6)
9 | 0.35 BARE | 514 | Ground (UE1) | 9 | 0.35 BARE | 514 | Ground (UE1)
10 | 0.35 GY | 655 | Cellular Microphone Signal (UE1) | 10 | 0.35 GY | 655 | Cellular Microphone Signal (UE1)
11-12 | -- | -- | Not Used | 11-12 | -- | -- | Not Used
13 | 0.5 GY/BK | 690 | Courtesy Lamp High Control | 13 | 0.8 GY/BK | 690 | Courtesy Lamp High Control
14 | 0.35 L-BU | 5304 | Front Sunshade Switch Open Signal (C3U) | 14 | 0.35 L-BU | 5304 | Front Sunshade Switch Open Signal (C3U)
15 | 0.35 YE | 5305 | Front Sunshade Switch Close Signal (C3U) | 15 | 0.35 YE | 5305 | Front Sunshade Switch Close Signal (C3U)
16 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (C3U or UG1) | 16 | 0.5 GY | 8 | Instrument Panel Lamp Voltage (C3U or UG1)

### X351 Rear HVAC Harness to Body Harness

#### Connector Part Information

- OEM: 88986335
- Service: 88986267
- Description: 12-Way F GT Mixed (BK)

#### Connector Part Information

- OEM: 88986319
- Service: 88986259
- Description: 12-Way M GT Mixed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: B-E, H, J-K
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: F-G
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: A, M
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins: M : A/D
- Core/Insulation Crimp: Pins: A : C/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X351 Rear HVAC Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 RD/WH | 2640 | Battery Positive Voltage | A | 2 RD/WH | 2640 | Battery Positive Voltage
B | 0.35 L-BN | 5729 | Auxiliary Mode Motor Voltage | B | 0.5 L-GN/WH | 5729 | Auxiliary Mode Motor Voltage
C | 0.35 OG | 2215 | Auxiliary Mode Door Control | C | 0.5 OG | 2215 | Auxiliary Mode Door Control
D | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control | D | 0.5 GY | 2614 | Auxiliary Air Temperature Door Control
E | 0.35 GY | 2599 | Auxiliary Mode Door Control | E | 0.5 GY | 2599 | Auxiliary Mode Door Control
F | 0.35 GY | 596 | 5-Volt Reference | F | 0.5 GY | 596 | 5-Volt Reference
0.35 GY | 596 | 5-Volt Reference
G | 0.35 GY/BK | 1798 | Low Reference | G | 0.5 GY/BK | 1798 | Low Reference
0.35 GY/BK | 1798 | Low Reference
H | 0.35 PK | 2145 | Air Temperature Switch Signal - Right | H | 0.5 PK | 2145 | Air Temperature Switch Signal - Right
J | 0.35 D-GN | 2211 | Auxiliary Blower Motor Speed Control | J | 0.5 D-GN | 2211 | Auxiliary Blower Motor Speed Control
K | 0.35 BN | 6555 | Auxiliary Temperature Motor Voltage | K | 0.5 BN | 6555 | Auxiliary Temperature Motor Voltage
L | -- | -- | Not Used | L | -- | -- | Not Used
M | 3 BK | 850 | Ground | M | 3 BK | 850 | Ground

### X380 Body Harness to Auxiliary Power Outlet - Rear Console Harness (DK1)

#### Connector Part Information

- OEM: 7283-5548-30
- Service: 88953306
- Description: 2-Way F YESC Weather Pack (BK)

#### Connector Part Information

- OEM: 7282-5548-30
- Service: 88953303
- Description: 2-Way M YESC Weather Pack (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X380 Body Harness to Auxiliary Power Outlet - Rear Console Harness (DK1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 RD/WH | 140 | Battery Positive Voltage | 1 | 1 RD/WH | 140 | Battery Positive Voltage
2 | 1 BK | 750 | Ground | 2 | 1 BK | 750 | Ground

### X398 Headliner Harness to Sunroof Harness (C3U)

#### Connector Part Information

- OEM: 7283-6459-40
- Service: See Catalog
- Description: 10-Way F YESC Kaizen Series, Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-5621-40
- Service: See Catalog
- Description: 10-Way M YESC Kaizen Series, Unsealed (L-GY)

#### Terminal Part Information

- Pins: 1, 5
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

- Pins: 2-3, 7-8
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pin: 6
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 1, 5
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 2, 3, 7-10
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 6
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X398 Headliner Harness to Sunroof Harness (C3U)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 3 BK | 850 | Ground | 1 | 3 BK | 850 | Ground
2 | 0.35 BN | 100 | Sunroof Switch Open Signal | 2 | 0.35 BN | 100 | Sunroof Switch Open Signal
3 | 0.35 OG | 110 | Sunroof Switch Close Signal | 3 | 0.35 OG | 110 | Sunroof Switch Close Signal
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 3 RD/WH | 3440 | Battery Positive Voltage | 5 | 3 RD/WH | 3440 | Battery Positive Voltage
6 | 0.35 YE | 43 | Ignition Voltage | 6 | 0.35 YE | 43 | Ignition Voltage
7 | 0.35 L-BU | 5304 | Front Sunshade Switch Open Signal | 7 | 0.35 D-BU | 5304 | Front Sunshade Switch Open Signal
8 | 0.35 YE | 5305 | Front Sunshade Switch Close Signal | 8 | 0.35 YE/BK | 5305 | Front Sunshade Switch Close Signal
9-10 | -- | -- | Not Used | 9 | PU | -- | Serial Communication
10 | WH | -- | Serial Communication

### X405 Rear Chassis Harness to Body Harness

#### Connector Part Information

- OEM: 12176335
- Service: See Catalog
- Description: 8-Way F Metri-Pack Mixed Series, Sealed (L-GY)

- OEM: 12162144
- Service: 12102741
- Description: 4-Way F 150 Metri-Pack Series, Sealed (L-GY)

- OEM: 12146439
- Service: 12146439
- Description: 4-Way F 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 13609624
- Service: See Catalog
- Description: 16-Way M Metri-Pack Mixed Series, Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 1A, 1B, 1C, 1D, 2A, 2B
- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

- Pins: 3A-3E, 3G-3H
- Terminal/Tray: 12048159/2
- Core/Insulation Crimp: Pins: 3C : See Terminal Repair Kit
- Core/Insulation Crimp: Pins: 3B, 3D : 2/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X405 Rear Chassis Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal | 1A | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
B | 0.5 WH | 883 | Low Reference | 1B | 0.5 WH | 883 | Low Reference
C | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal | 1C | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
D | 0.5 OG | 885 | Low Reference | 1D | 0.5 OG | 885 | Low Reference
A | 0.5 RD/WH | 1740 | Battery Positive Voltage (MH6) | 2A | 0.5 RD/WH | 1740 | Battery Positive Voltage (MH6)
B | 0.5 BK | 650 | Ground (MH6) | 2B | 0.5 BK | 650 | Ground (MH6)
C-D | -- | -- | Not Used | 2C-2D | -- | -- | Not Used
A | 3 RD/WH | 2940 | Battery Positive Voltage | 3A | 3 RD/WH | 2940 | Battery Positive Voltage
B | 0.35 PK | 439 | Ignition Voltage | 3B | 0.35 PK | 439 | Ignition Voltage
C | 0.35 L-BU | 5986 | Communication Enable (MH6) | 3C | 0.35 L-BU | 5986 | Communication Enable (MH6)
D | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | 3D | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
E | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus- | 3E | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
F | -- | -- | Not Used | 3F | -- | -- | Not Used
G | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control | 3G | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control
H | 3 BK | 650 | Ground | 3H | 3 BK | 650 | Ground

### X440 Body Harness to Rear Bumper Harness (UD7 or X88)

#### Connector Part Information

- OEM: 7283-5946-30
- Service: See Catalog
- Description: 10-Way F YESC/USCAR Class III Series (BK)

#### Connector Part Information

- OEM: 7282-5946-30
- Service: See Catalog
- Description: 10-Way M YESC/USCAR Class III Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### X440 Body Harness to Rear Bumper Harness (UD7 or X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 D-BU | 2374 | Object Sensor Voltage (UD7) | 1 | 0.35 D-BU | 2374 | Object Sensor Voltage (UD7)
2 | 0.5 PU | 709 | Park Lamp Voltage (X88) | 2 | 0.5 PU | 709 | Park Lamp Voltage (X88)
3 | 0.35 YE | 2375 | LR Corner Object Sensor Signal (UD7) | 3 | 0.35 YE | 2375 | LR Corner Object Sensor Signal (UD7)
4 | 0.35 OG | 2376 | LR Middle Object Sensor Signal (UD7) | 4 | 0.35 OG | 2376 | LR Middle Object Sensor Signal (UD7)
5 | 0.35 D-GN | 2377 | RR Middle Object Sensor Signal (UD7) | 5 | 0.35 D-GN | 2377 | RR Middle Object Sensor Signal (UD7)
6 | 0.5 BK | 650 | Ground (X88) | 6 | 0.5 BK | 650 | Ground (X88)
7 | 0.35 GY | 2379 | Low Reference (UD7) | 7 | 0.35 GY | 2379 | Low Reference (UD7)
8 | 0.35 PU | 2378 | RR Corner Object Sensor Signal (UD7) | 8 | 0.35 PU | 2378 | RR Corner Object Sensor Signal (UD7)
9-10 | -- | -- | Not Used | 9-10 | -- | -- | Not Used

### X442 Body Harness to Trailer Harness (V92)

#### Connector Part Information

- OEM: 7283-5574-10
- Service: See Catalog
- Description: 8-Way F 2.8 Series, Sealed (D-GY)

#### Connector Part Information

- OEM: 7282-5574-10
- Service: See Catalog
- Description: 8-Way M 2.8 Series, Sealed (D-GY)

#### Terminal Part Information

- Pins: 2-4, 6, 8
- Terminal/Tray: 7116-4150-02/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 5, 8
- Terminal/Tray: 7116-4152-02/9
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 2-4, 6, 8
- Terminal/Tray: 7114-4150-02/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1, 5, 8
- Terminal/Tray: 7114-4152-02/9
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X442 Body Harness to Trailer Harness (V92)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 RD/BK | 542 | Battery Positive Voltage (V92) | 1 | 2 RD/BK | 542 | Battery Positive Voltage (V92)
2 | 0.5 YE | 1618 | Stop Lamp Voltage | 2 | 0.5 YE | 1618 | Stop Lamp Voltage
3 | 0.5 L-GN | 1624 | Trailer Backup Lamps Voltage (V92) | 3 | 0.5 L-GN | 1624 | Trailer Backup Lamps Voltage (V92)
4 | 0.5 BN | 2109 | Trailer Park Lamps Voltage | 4 | 0.5 BN | 2109 | Trailer Park Lamps Voltage
5 | 2 D-BU | 47 | Trailer Auxiliary Voltage (V92) | 5 | 2 D-BU | 47 | Trailer Auxiliary Voltage (V92)
6 | 0.5 D-GN | 1619 | Stop Lamp Voltage | 6 | 0.5 D-GN | 1619 | Stop Lamp Voltage
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | 2 BK | 850 | Ground (V92) | 8 | 2 BK | 850 | Ground (V92)
0.5 BK | 850 | Ground (without V92) | 0.5 BK | 850 | Ground (without V92)

### X450 Body Harness to Right Tail Lamp Harness (W49 or X88)

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177532
- Service: 15326813
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, C : 2/A
- Core/Insulation Crimp: Pins: B : E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X450 Body Harness to Right Tail Lamp Harness (W49 or X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 D-GN | 19 | Right Rear Stop/Turn Lamp Voltage | A | 0.8 WH | -- | Right Rear Stop/Turn Lamp Voltage (W49)
0.8 RD | -- | Right Rear Stop/Turn Lamp Voltage (X88)
B | 0.5 BN/WH | 309 | Right Park Lamp Voltage | B | 0.5 D-BU | -- | Right Park Lamp Voltage (W49)
0.8 L-BU | -- | Right Park Lamp Voltage (X88)
C | 0.8 BK | 850 | Ground | C | 0.8 BK | -- | Ground

### X450 Body Harness to Right Tail Lamp Harness (WDA)

#### Connector Part Information

- OEM: 33471-0301
- Service: See Catalog
- Description: 3-Way F MX150 Series (BK)

#### Connector Part Information

- OEM: 33481-0301
- Service: See Catalog
- Description: 3-Way M MX150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 33012-1002/26
- Core/Insulation Crimp: Pins: 2 : E/C
- Core/Insulation Crimp: Pins: 1, 3 : 2/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X450 Body Harness to Right Tail Lamp Harness (WDA)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 850 | Ground | 1 | BK | -- | Ground
2 | 0.5 BN/WH | 309 | Right Park Lamp Voltage | 2 | L-BU | -- | Right Park Lamp Voltage
3 | 0.8 D-GN | 19 | Right Rear Stop/Turn Lamp Voltage | 3 | RD | -- | Right Rear Stop/Turn Lamp Voltage

### X451 Body Harness to Left Tail Lamp Harness (W49 or X88)

#### Connector Part Information

- OEM: 15326808
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177532
- Service: 15326813
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A, C : 2/A
- Core/Insulation Crimp: Pins: B : E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X451 Body Harness to Left Tail Lamp Harness (W49 or X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 YE | 18 | Left Rear Stop/Turn Lamp Voltage | A | 0.8 WH | -- | Left Rear Stop/Turn Lamp Voltage (W49)
0.8 RD | -- | Left Rear Stop/Turn Lamp Voltage (X88)
B | 0.5 PU | 709 | Left Park Lamp Voltage | B | 0.5 D-BU | -- | Left Park Lamp Voltage (W49)
0.8 L-BU | -- | Left Park Lamp Voltage (X88)
C | 0.8 BK | 650 | Ground | C | 0.8 BK | -- | Ground

### X451 Body Harness to Left Tail Lamp Harness (WDA)

#### Connector Part Information

- OEM: 33471-0301
- Service: See Catalog
- Description: 3-Way F MX150 Series (BK)

#### Connector Part Information

- OEM: 33481-0301
- Service: See Catalog
- Description: 3-Way M MX150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 33012-1002/26
- Core/Insulation Crimp: Pins: 2 : E/C
- Core/Insulation Crimp: Pins: 1, 3 : 2/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X451 Body Harness to Left Tail Lamp Harness (WDA)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 650 | Ground | 1 | BK | -- | Ground
2 | 0.5 PU | 709 | Left Park Lamp Voltage | 2 | L-BU | -- | Left Park Lamp Voltage
3 | 0.8 YE | 18 | Left Rear Stop/Turn Lamp Voltage | 3 | RD | -- | Left Rear Stop/Turn Lamp Voltage

### X500 Driver Door Harness to Body Harness

#### Connector Part Information

- OEM: 6098-5138
- Service: See Catalog
- Description: 40-Way F Sealed (BK)

#### Connector Part Information

- OEM: 6098-5850
- Service: See Catalog
- Description: 40-Way M Sealed (BK)

#### Terminal Part Information

- Pins: 1-14, 16, 25, 27-39
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 17-22, 24, 26
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins: 17, 19, 22, 24, 26 : 2/A
- Core/Insulation Crimp: Pins: 18, 20-21 : E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 15, 23
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: Pins: 23 : 4/4
- Core/Insulation Crimp: Pins: 15, 23 : F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 1-14, 16, 25, 27-39
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins: 5, 7, 8, 27 : E/4
- Core/Insulation Crimp: Pins: 1-4, 6, 9-14, 16, 25, 27-39 : E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 18, 20-21
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: 15, 17, 19, 22-24, 26
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins: 17, 19, 22, 24, 26 : 2/A
- Core/Insulation Crimp: Pins: 15, 23 : A/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X500 Driver Door Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal (without AXC or AXE) | 1 | 0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal (without AXC or AXE)
2 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (A45 with KA1 or KB6) | 2 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (A45 with KA1 or KB6)
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.5 GY/BK | 745 | Left Front Door Ajar Switch Signal (without AXC or AXE) | 4 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal (without AXC or AXE)
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal (without AXC or AXE) | 6 | 0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal (without AXC or AXE)
7 | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage (DNP or DNT or DS3) | 7 | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage (DNP or DNT or DS3)
8 | 0.5 OG | 2267 | Mirror Heating Element Voltage (DS3) | 8 | 0.5 OG | 2267 | Mirror Heating Element Voltage (DS3)
9 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (A45 with KA1 or KB6) | 9 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (A45 with KA1 or KB6)
10 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control (DL6 or DS3) | 10 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control (DL6 or DS3)
11 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (without AXC or AXE) | 11 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (without AXC or AXE)
12 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control (DL6 or DS3) | 12 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control (DL6 or DS3)
13 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (without AXC or AXE) | 13 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (without AXC or AXE)
14 | 0.35 TN/WH | 330 | Passenger Mirror Motor Voltage (DL6 or DS3) | 14 | 0.35 TN/WH | 330 | Passenger Mirror Motor Voltage (DL6 or DS3)
15 | 3 BK | 550 | Ground | 15 | 3 BK | 550 | Ground
16 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6) | 16 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6)
17 | 1 RD/WH | 3240 | Battery Positive Voltage (AXC or AXE) | 17 | 1 RD/WH | 3240 | Battery Positive Voltage (AXC or AXE)
18 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6) | 18 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6)
19 | 0.8 GY | 118 | Left Front Speaker Output (-) | 19 | 0.8 GY | 118 | Left Front Speaker Output (-)
20 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (A45 with KA1 or KB6) | 20 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (A45 with KA1 or KB6)
21 | 0.5 RD/WH | 1940 | Battery Positive Voltage (DL6 or DS3) | 21 | 0.5 RD/WH | 1940 | Battery Positive Voltage (DL6 or DS3)
22 | 0.8 TN | 201 | Left Front Speaker Output (+) | 22 | 1 TN | 201 | Left Front Speaker Output (+)
23 | 3 RD/WH | 3340 | Battery Positive Voltage (without AXC or AXE) | 23 | 3 RD/WH | 3340 | Battery Positive Voltage
2 RD/WH | 3340 | Battery Positive Voltage (AXC or AXE)
24 | 0.8 TN | 694 | Driver Door Lock Actuator Unlock Control (without AXC or AXE) | 24 | 1 TN | 694 | Driver Door Lock Actuator Unlock Control (without AXC or AXE)
25 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6) | 25 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6)
26 | 0.8 GY | 295 | Door Lock Actuator Lock Control (without AXC or AXE) | 26 | 1 GY | 295 | Door Lock Actuator Lock Control (without AXC or AXE)
27 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6) | 27 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6)
0.35 GY | 8 | Instrument Panel Lamp Voltage (without AXC or AXE or DL6 or DS3) | 0.5 GY | 8 | Instrument Panel Lamp Voltage (without AXC or AXE or DL6 or DS3)
28 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE) | 28 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE)
29 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE) | 29 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE)
30 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP) | 30 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP)
31 | 0.35 PK | 1691 | Low Reference (DNP) | 31 | 0.35 PK | 1691 | Low Reference (DNP)
32 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal | 32 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal
33 | 0.35 PU/WH | 6628 | Low Reference | 33 | 0.35 PU/WH | 6628 | Low Reference
34 | 0.5 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (without AXC or AXE) | 34 | 0.35 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (without AXC or AXE)
35 | 0.5 PK/BK | 780 | Driver Door Lock Switch Lock Signal (without AXC or AXE) | 35 | 0.35 PK/BK | 780 | Driver Door Lock Switch Lock Signal (without AXC or AXE)
36 | 0.35 PU/WH | 1382 | LED Dimming Signal (without AXC or AXE) | 36 | 0.35 PU/WH | 1382 | LED Dimming Signal (without AXC or AXE)
0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE) | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE)
37 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (without AXC or AXE) | 37 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (without AXC or AXE)
38 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE) | 38 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE)
39 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (without AXC or AXE) | 39 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (without AXC or AXE)
40 | -- | -- | Not Used | 40 | -- | -- | Not Used

### X553 Driver Door Trim Panel Harness to Driver Door Harness

#### Connector Part Information

- OEM: 7283-6457-40
- Service: See Catalog
- Description: 10-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-6457-40
- Service: See Catalog
- Description: 10-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Pins: 2-4, 6-10
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 5
- Terminal/Tray: 7116-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 5, 7, 9
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 5
- Terminal/Tray: 7114-4111-02/9
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 2-4, 6-10
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1, 5, 7, 9
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X553 Driver Door Trim Panel Harness to Driver Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 BK | 550 | Ground (AXC or AXE) | 1 | 3 BK | 550 | Ground
3 BK | 550 | Ground (without AXC or AXE)
2 | 0.5 RD/WH | 1940 | Battery Positive Voltage (DL6 or DS3) | 2 | 0.5 RD/WH | 1940 | Battery Positive Voltage (DL6 or DS3)
3 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (A45 with KA1 or KB6) | 3 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (A45 with KA1 or KB6)
4 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control (DL6 or DS3) | 4 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control (DL6 or DS3)
0.35 PU | 6174 | Driver Heated Seat Switch Back LED (A45 with KA1 or KB6) | 0.35 PU | 6174 | Driver Heated Seat Switch Back LEDl (A45 with KA1 or KB6)
5 | 1 RD/WH | 3240 | Battery Positive Voltage (AXC or AXE) | 5 | 1 RD/WH | 3240 | Battery Positive Voltage (AXC or AXE)
3 RD/WH | 3340 | Battery Positive Voltage (without AXC or AXE) | 3 RD/WH | 3340 | Battery Positive Voltage (without AXC or AXE)
6 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control (DL6 or DS3) | 6 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control (DL6 or DS3)
0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6) | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6)
7 | 3 BN | 165 | Power Window Motor Left Front Down Control (without AXC or AXE) | 7 | 3 BN | 165 | Power Window Motor Left Front Down Control (without AXC or AXE)
0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AXC or AXE) | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AXC or AXE)
8 | 0.35 TN/WH | 330 | Passenger Mirror Motor Voltage (DL6 or DS3) | 8 | 0.35 TN/WH | 330 | Passenger Mirror Motor Voltage (DL6 or DS3)
0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (A45 with KA1 or KB6) | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (A45 with KA1 or KB6)
9 | 3 D-BU | 164 | Power Window Motor Left Front Up Control (without AXC or AXE) | 9 | 3 D-BU | 164 | Power Window Motor Left Front Up Control (without AXC or AXE)
0.5 GY | 295 | Door Lock Actuator Lock Control (AXC or AXE) | 0.5 GY | 295 | Door Lock Actuator Lock Control (AXC or AXE)
10 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (DL6 or DS3 without AXC or AXE) | 10 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (DL6 or DS3 without AXC or AXE)

### X555 Driver Door Trim Panel Harness to Driver Door Harness

#### Connector Part Information

- OEM: 7283-6453-60
- Service: See Catalog
- Description: 16-Way F Kaizen YESC Series, Unsealed (GN)

#### Connector Part Information

- OEM: 7282-6453-60
- Service: See Catalog
- Description: 16-Way M Kaizen YESC Series (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X555 Driver Door Trim Panel Harness to Driver Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 TN | 329 | Driver Mirror Motor Voltage (DL6 or DS3) | 1 | 0.35 TN | 329 | Driver Mirror Motor Voltage (DL6 or DS3)
2 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP) | 2 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP)
0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal (without AXC or AXE) | 0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal (without AXC or AXE)
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.35 WH | 81 | Driver Mirror Motor Right Control (DL6 or DS3) | 4 | 0.35 WH | 81 | Driver Mirror Motor Right Control (DL6 or DS3)
5 | 0.35 L-GN | 89 | Left Mirror Motor Down Control (DL6 or DS3) | 5 | 0.35 L-GN | 89 | Left Mirror Motor Down Control (DL6 or DS3)
0.5 GY/BK | 745 | Left Front Door Ajar Switch Signal (AXC or AXE) | 0.5 GY/BK | 745 | Left Front Door Ajar Switch Signal (AXC or AXE)
6 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE) | 6 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE)
0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6) | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6)
7 | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage (A45 with DNP or DNT or DS3) | 7 | 0.5 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage (A45 with DNP or DNT or DS3)
0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE) | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE)
8 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (without AXC or AXE) | 8 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (without AXC or AXE)
9 | 0.35 PK | 1691 | Low Reference (DNP) | 9 | 0.35 PK | 1691 | Low Reference (DNP)
0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE) | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE)
10 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6) | 10 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6)
0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (without AXC or AXE) | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (without AXC or AXE)
11 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE) | 11 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE)
0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal (without AXC or AXE) | 0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal (without AXC or AXE)
12 | 0.5 YE | 5942 | Low Reference (AXC or AXE) | 12 | 0.5 YE | 5942 | Low Reference (AXC or AXE)
0.35 PU/WH | 1382 | LED Dimming Signal (without AXC or AXE) | 0.35 PU/WH | 1382 | LED Dimming Signal (without AXC or AXE)
13 | 0.35 BN | 6132 | Linear Interconnect Network Bus (AXC or AXE) | 13 | 0.35 BN | 6132 | Linear Interconnect Network Bus (AXC or AXE)
0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (without AXC or AXE) | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (without AXC or AXE)
14 | 0.5 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (without AXC or AXE) | 14 | 0.5 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (without AXC or AXE)
15 | 0.5 PK/BK | 780 | Driver Door Lock Switch Lock Signal (without AXC or AXE) | 15 | 0.5 PK/BK | 780 | Driver Door Lock Switch Lock Signal (without AXC or AXE)
0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6) | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6)
16 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (without AXC or AXE) | 16 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (without AXC or AXE)

### X600 Passenger Door Harness to Body Harness

#### Connector Part Information

- OEM: 6098-5138
- Service: See Catalog
- Description: 40-Way F Sealed (BK)

#### Connector Part Information

- OEM: 6098-5850
- Service: See Catalog
- Description: 40-Way M Sealed (BK)

#### Terminal Part Information

- Pins: 3-8, 10-14, 16, 25, 27-29, 32-36, 38
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 19, 21-22, 24, 26
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 15, 17
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 3-8, 27, 10-14, 16, 27-29, 32-36, 38
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins: 4 : 2/4
- Core/Insulation Crimp: Pins: 7-8, 27 : E/4
- Core/Insulation Crimp: Pins: 3-6, 10-14, 16, 27-29, 32-36, 38 : E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 15, 17, 19, 21-22, 24, 26
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins: 19, 21-22, 24, 26 : 2/A
- Core/Insulation Crimp: Pins: 15, 17 : C/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: 25
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### X600 Passenger Door Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-3 | -- | -- | Not Used | 1-3 | -- | -- | Not Used
4 | 0.5 TN/WH | 746 | Right Front Door Ajar Switch Signal (without AXC or AXE) | 4 | 0.5 TN/WH | 746 | Right Front Door Ajar Switch Signal (without AXC or AXE)
5 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6) | 5 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6)
6 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (A45 with KA1 or KB6) | 6 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (A45 with KA1 or KB6)
7 | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage (DNP or DNT or or DS3) | 7 | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage (DNP or DNT or DS3)
8 | 0.5 OG | 2267 | Mirror Heating Element Voltage (DS3) | 8 | 0.5 OG | 2267 | Mirror Heating Element Voltage (DS3)
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control (DL6 or DS3) | 10 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control (DL6 or DS3)
11 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (A45 with KA1 or KB6) | 11 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (A45 with KA1 or KB6)
12 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control (DL6 or DS3) | 12 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control (DL6 or DS3)
13 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (A45 with KA1 or KB6) | 13 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (A45 with KA1 or KB6)
14 | 0.35 TN/WH | 330 | Passenger Mirror Motor Voltage (DL6 or DS3) | 14 | 0.35 TN/WH | 330 | Passenger Mirror Motor Voltage (DL6 or DS3)
15 | 2 BK | 750 | Ground | 15 | 2 BK | 750 | Ground
16 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6) | 16 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6)
17 | 2 RD/WH | 3340 | Battery Positive Voltage | 17 | 2 RD/WH | 3340 | Battery Positive Voltage
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | 0.8 D-GN | 117 | Right Front Speaker Output (-) | 19 | 0.8 D-GN | 117 | Right Front Speaker Output (-)
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | 0.8 RD/WH | 840 | Battery Positive Voltage (AXC or AXE) | 21 | 0.8 RD/WH | 840 | Battery Positive Voltage (AXC or AXE)
22 | 0.8 L-GN | 200 | Right Front Speaker Output (+) | 22 | 0.8 L-GN | 200 | Right Front Speaker Output (+)
23 | -- | -- | Not Used | 23 | -- | -- | Not Used
24 | 0.8 TN | 294 | Door Lock Actuator Unlock Control (without AXC or AXE) | 24 | 1 TN | 294 | Door Lock Actuator Unlock Control (without AXC or AXE)
25 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6) | 25 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6)
26 | 0.8 GY | 295 | Door Lock Actuator Lock Control (without AXC or AXE) | 26 | 1 GY | 295 | Door Lock Actuator Lock Control (without AXC or AXE)
27 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (without AXC or AXE) | 27 | 0.5 GY | 8 | Instrument Panel Lamp Voltage (without AXC or AXE)
0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6) | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6)
28 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE) | 28 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE)
29 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE) | 29 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE)
30-31 | -- | -- | Not Used | 30-31 | -- | -- | Not Used
32 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal | 32 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal
33 | 0.35 WH/BK | 6629 | Low Reference | 33 | 0.35 WH/BK | 6629 | Low Reference
34 | 0.5 D-BU | 245 | Passenger Door Lock Switch Unlock (without AXC or AXE) | 34 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock (without AXC or AXE)
35 | 0.5 L-BU | 244 | Passenger Door Lock Switch Lock (without AXC or AXE) | 35 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock (without AXC or AXE)
36 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE) | 36 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE)
37 | -- | -- | Not Used | 37 | -- | -- | Not Used
38 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE) | 38 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE)
39-40 | -- | -- | Not Used | 39-40 | -- | -- | Not Used

### X664 Passenger Door Trim Panel Harness to Passenger Door Harness

#### Connector Part Information

- OEM: 7283-6457-40
- Service: See Catalog
- Description: 10-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-6457-40
- Service: See Catalog
- Description: 10-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Pins: 2-4, 6, 8, 10
- Terminal/Tray: 7116-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 5, 7, 9
- Terminal/Tray: 7116-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-35 (VT)

#### Terminal Part Information

- Pins: 2-4, 6, 8, 10
- Terminal/Tray: 7114-4110-02/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: 1, 5, 7, 9
- Terminal/Tray: 7114-4112-02/9
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X664 Passenger Door Trim Panel Harness to Passenger Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 RD/WH | 3340 | Battery Positive Voltage (without AXC) | 1 | 2 RD/WH | 3340 | Battery Positive Voltage (without AXC)
2 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6) | 2 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6)
3 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (without AXC or AXE) | 3 | 0.35 GY | 8 | Instrument Panel Lamp Voltage (without AXC or AXE)
0.5 GY | 295 | Door Lock Actuator Lock Control (AXC or AXE) | 0.5 GY | 295 | Door Lock Actuator Lock Control (AXC or AXE)
4 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (A45 with KA1 or KB6) | 4 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED (A45 with KA1 or KB6)
5 | 2 BK | 750 | Ground | 5 | 2 BK | 750 | Ground
6 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (A45 with KA1 or KB6) | 6 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal (A45 with KA1 or KB6)
7 | 2 BN | 667 | Power Window Motor Right Front Down Control (without AXC) | 7 | 2 BN | 667 | Power Window Motor Right Front Down Control (without AXC)
8 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AXC or AXE) | 8 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AXC or AXE)
9 | 2 D-BU | 666 | Power Window Motor Right Front Up Control (without AXC) | 9 | 2 D-BU | 666 | Power Window Motor Right Front Up Control (without AXC)
10 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (A45 with KA1 or KB6) | 10 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (A45 with KA1 or KB6)

### X666 Passenger Door Trim Panel Harness to Passenger Door Harness

#### Connector Part Information

- OEM: 7283-6453-60
- Service: See Catalog
- Description: 16-Way F Kaizen YESC Series, Unsealed (GN)

#### Connector Part Information

- OEM: 7282-6453-60
- Service: See Catalog
- Description: 16-Way M Kaizen YESC Series (GN)

#### Terminal Part Information

- Pins: 1, 3-8, 11-16
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 10
- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 10
- Terminal/Tray: 7114-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1, 3-8, 11-16
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X666 Passenger Door Trim Panel Harness to Passenger Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE) | 1 | 0.35 YE | 43 | Ignition Voltage (without AXC or AXE)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | 0.5 TN/WH | 746 | Right Front Door Ajar Switch Signal (AXC or AXE) | 3 | 0.5 TN/WH | 746 | Right Front Door Ajar Switch Signal (AXC or AXE)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage (DNP or DNT or DS3) | 5 | 0.5 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage (DNP or DNT or DS3)
6 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6) | 6 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6)
7 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6) | 7 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6)
8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE) | 8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (without AXC or AXE)
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | 0.8 RD/WH | 840 | Battery Positive Voltage (AXC or AXE) | 10 | 0.8 RD/WH | 840 | Battery Positive Voltage (AXC or AXE)
11 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE) | 11 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (AXC or AXE)
12 | 0.5 YE | 5943 | Low Reference (AXC or AXE) | 12 | 0.5 YE | 5943 | Low Reference (AXC or AXE)
0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE) | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (without AXC or AXE)
13 | 0.35 D-BU | 6133 | Linear Interconnect Network Bus (AXC) | 13 | 0.35 D-BU | 6133 | Linear Interconnect Network Bus (AXC)
14 | 0.5 L-BU | 244 | Passenger Door Lock Switch Lock (without AXC or AXE) | 14 | 0.5 L-BU | 244 | Passenger Door Lock Switch Lock (without AXC or AXE)
15 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6) | 15 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6)
16 | 0.5 D-BU | 245 | Passenger Door Lock Switch Unlock (without AXC or AXE) | 16 | 0.5 D-BU | 245 | Passenger Door Lock Switch Unlock (without AXC or AXE)

### X700 Left Rear Door Harness to Body Harness

#### Connector Part Information

- OEM: 6098-5144
- Service: See Catalog
- Description: 19-Way F Sealed (BK)

#### Connector Part Information

- OEM: 6098-5141
- Service: See Catalog
- Description: 19-Way M Sealed (BK)

#### Terminal Part Information

- Pins: 9-18
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins: 17-18 : C/A
- Core/Insulation Crimp: Pins: 9-16 : E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 4-5
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 1, 8
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 9-18
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins: 17-18 : 2/4
- Core/Insulation Crimp: Pins: 17-18 : E/4
- Core/Insulation Crimp: Pins: 9-16 : E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1, 4-5, 8
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins: 4-5 : 2/A
- Core/Insulation Crimp: Pins: 1, 8 : C/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X700 Left Rear Door Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 RD/WH | 3340 | Battery Positive Voltage | 1 | 2 RD/WH | 3340 | Battery Positive Voltage
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | 0.8 GY | 295 | Door Lock Actuator Lock Control | 4 | 1 GY | 295 | Door Lock Actuator Lock Control
5 | 0.8 TN | 294 | Door Lock Actuator Unlock Control | 5 | 1 TN | 294 | Door Lock Actuator Unlock Control
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | 2 BK | 550 | Ground | 8 | 2 BK | 550 | Ground
9 | 0.5 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal | 9 | 0.35 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | 0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal | 11 | 0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal
12 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal | 12 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
13 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal | 13 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
14 | 0.35 L-BU | 6622 | Left Rear Side Impact Sensing Module Signal | 14 | 0.35 L-BU | 6622 | Left Rear Side Impact Sensing Module Signal
15 | 0.35 L-GN/BK | 6623 | Low Reference | 15 | 0.35 L-GN/BK | 6623 | Low Reference
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | 0.8 YE | 116 | Left Rear Speaker Output (-) | 17 | 0.8 YE | 116 | Left Rear Speaker Output (-) (UQA or UQS)
0.5 YE | 116 | Left Rear Speaker Output (-) (UQF)
18 | 0.8 BN | 199 | Left Rear Speaker Output (+) | 18 | 0.8 BN | 199 | Left Rear Speaker Output (+) (UQA or UQS)
0.5 BN | 199 | Left Rear Speaker Output (+) (UQF)
19 | -- | -- | Not Used | 19 | -- | -- | Not Used

### X800 Right Rear Door Harness to Body Harness

#### Connector Part Information

- OEM: 6098-5144
- Service: See Catalog
- Description: 19-Way F Sealed (BK)

#### Connector Part Information

- OEM: 6098-5141
- Service: See Catalog
- Description: 19-Way M Sealed (BK)

#### Terminal Part Information

- Pins: 9-18
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins: 17, 18 : C/A
- Core/Insulation Crimp: Pins: 9-16 : E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 4, 5
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 1, 8
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: 9-18
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins: 17, 18 : 2/4
- Core/Insulation Crimp: Pins: 17, 18 : E/4
- Core/Insulation Crimp: Pins: 9-16 : E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: 1, 4, 5, 8
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins: 4, 5 : 2/A
- Core/Insulation Crimp: Pins: 1, 8 : C/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X800 Right Rear Door Harness to Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2 RD/WH | 3340 | Battery Positive Voltage | 1 | 2 RD/WH | 3340 | Battery Positive Voltage
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | 0.8 GY | 295 | Door Lock Actuator Lock Control | 4 | 1 GY | 295 | Door Lock Actuator Lock Control
5 | 0.8 TN | 294 | Door Lock Actuator Unlock Control | 5 | 1 TN | 294 | Door Lock Actuator Unlock Control
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | 2 BK | 750 | Ground | 8 | 2 BK | 750 | Ground
9 | 0.5 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal | 9 | 0.35 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal | 11 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal
12 | 0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal | 12 | 0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal
13 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal | 13 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal
14 | 0.35 L-BU/WH | 6626 | Right Rear Side Impact Sensing Module Signal | 14 | 0.35 L-BU/WH | 6626 | Right Rear Side Impact Sensing Module Signal
15 | 0.35 PK/BK | 6627 | Low Reference | 15 | 0.35 PK/BK | 6627 | Low Reference
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | 0.8 L-BU | 115 | Right Rear Speaker Output (-) | 17 | 0.8 L-BU | 115 | Right Rear Speaker Output (-) (UQA or UQS)
0.5 L-BU | 115 | Right Rear Speaker Output (-) (UQF)
18 | 0.8 D-BU | 46 | Right Rear Speaker Output (+) | 18 | 0.8 D-BU | 46 | Right Rear Speaker Output (+) (UQA or UQS)
0.5 D-BU | 46 | Right Rear Speaker Output (+) (UQF)
19 | -- | -- | Not Used | 19 | -- | -- | Not Used

### X901 Body Harness to Liftgate Harness

#### Connector Part Information

- OEM: 7283-3740-40
- Service: See Catalog
- Description: 6-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-5604-40
- Service: See Catalog
- Description: 6-Way M 6.3 YESC Series (L-GY)

#### Terminal Part Information

- Pins: 5-6
- Terminal/Tray: 7116-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 1, 3
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: Pins: 1 : A/B
- Core/Insulation Crimp: Pins: 3 : D/G
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 2, 4
- Terminal/Tray: 7116-4121-02/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Terminal Part Information

- Pins: 5-6
- Terminal/Tray: 7114-4120-02/9
- Core/Insulation Crimp: E/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 1, 3
- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: Pins: 1 : A/B
- Core/Insulation Crimp: Pins: 3 : D/G
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

- Pins: 2, 4
- Terminal/Tray: 7114-4121-02/9
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### X901 Body Harness to Liftgate Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 3 BK | 650 | Ground | 1 | 3 BK | 650 | Ground
2 | 2 BN | 5790 | Liftgate Cinch Latch Motor Open Control (TB5) | 2 | 2 BN | 5790 | Liftgate Cinch Latch Motor Open Control (TB5)
3 | 5 PU | 293 | Rear Defog Element Voltage | 3 | 5 PU | 293 | Rear Defog Element Voltage
4 | 2 L-BU | 5791 | Liftgate Cinch Latch Motor Close Control (TB5) | 4 | 2 L-BU | 5791 | Liftgate Cinch Latch Motor Close Control (TB5)
5 | 1 BK | 650 | Ground | 5 | 1 BK | 650 | Ground
6 | 1 RD/WH | 3840 | Battery Positive Voltage | 6 | 1 RD/WH | 3840 | Battery Positive Voltage

### X902 Body Harness to Liftgate Harness (UVC)

#### Connector Part Information

- OEM: 7283-6386-40
- Service: 88988116
- Description: 4-Way F 0.64mm YESC Unsealed (L-GY)

#### Connector Part Information

- OEM: 7282-6560-40
- Service: See Catalog
- Description: 4-Way M 0.64mm YESC Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4720-02/14
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X902 Body Harness to Liftgate Harness (UVC)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PK | 239 | Ignition Voltage | 1 | 0.35 PK | 239 | Ignition Voltage
2 | 0.35 BARE | 6974 | Shield Wire | 2 | 0.35 BARE | 6974 | Shield Wire
3 | 0.35 PK | 6972 | Camera Video Signal (+) | 3 | 0.35 PK | 6972 | Camera Video Signal (+)
4 | 0.35 L-BU | 6973 | Camera Video Signal (-) | 4 | 0.35 L-BU | 6973 | Camera Video Signal (-)

### X903 Body Harness to Liftgate Harness

#### Connector Part Information

- OEM: 7283-6453-60
- Service: See Catalog
- Description: 16-Way F Kaizen YESC Series, Unsealed (GN)

#### Connector Part Information

- OEM: 7282-6453-60
- Service: See Catalog
- Description: 16-Way M Kaizen YESC Series (GN)

#### Terminal Part Information

- Pins: 1-7, 9-16
- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: Pins: 1-7, 9-16 : E/C
- Core/Insulation Crimp: Pins: 2, 9 : E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 15
- Terminal/Tray: 33012-1002/26
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Terminal Part Information

- Pins: 1-7, 9-16
- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X903 Body Harness to Liftgate Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 GY/BK | 690 | Courtesy Lamp High Control | 1 | 0.5 GY/BK | 690 | Courtesy Lamp High Control
2 | 0.5 L-BU | 1320 | Stop Lamp Voltage | 2 | 0.5 L-BU | 1320 | Stop Lamp Voltage
3 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal (TB4) | 3 | 0.5 PK/BK | 1303 | Liftgate Ajar Switch Signal (TB4)
4 | 0.5 L-GN | 2270 | Rear Window Washer Relay Control | 4 | 0.5 L-GN | 2270 | Rear Window Washer Relay Control
5 | 0.35 WH | 2283 | Rear Wiper/Washer Switch Voltage (without X88) | 5 | 0.35 WH | 2283 | Rear Wiper/Washer Switch Voltage (without X88)
6 | 0.5 D-BU | 38 | Backup Lamp Relay Control (UVC) | 6 | 0.5 D-BU | 38 | Backup Lamp Relay Control (UVC)
7 | 0.5 GY | 391 | Rear Window Wiper Switch Signal | 7 | 0.5 GY | 391 | Rear Window Wiper Switch Signal
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | 0.8 L-GN | 24 | Backup Lamp Voltage | 9 | 0.5 L-GN | 24 | Backup Lamp Voltage
10 | 0.35 PU/WH | 5801 | Low Reference (TB5) | 10 | 0.35 PU/WH | 5801 | Low Reference (TB5)
0.35 GY | 5797 | Rear Closure Handle Switch Open Signal (TB4) | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal (TB4)
11 | 0.35 PK/BK | 6000 | Latch Ratchet Switch Signal (TB5) | 11 | 0.35 PK/BK | 6000 | Latch Ratchet Switch Signal (TB5)
12 | 0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal (TB5) | 12 | 0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal (TB5)
0.5 L-BU | 6128 | Ground (TB4) | 0.5 L-BU | 6128 | Ground (TB4)
13 | 0.35 D-GN | 5512 | Latch Sector Switch Signal (TB5) | 13 | 0.35 D-GN | 5512 | Latch Sector Switch Signal (TB5)
14 | 0.35 WH/BK | 6126 | Liftgate Object Sensor 2 Signal (TB5) | 14 | 0.35 WH/BK | 6126 | Liftgate Object Sensor 2 Signal (TB5)
15 | 0.5 PU | 709 | Left Park Lamp Voltage | 15 | 0.5 PU | 709 | Left Park Lamp Voltage
16 | 0.35 GY | 7000 | Latch Pawl Switch Signal (TB5) | 16 | 0.35 GY | 7000 | Latch Pawl Switch Signal (TB5)

### X911 Liftgate Harness to Center High Mounted Stop Lamp (CHMSL) Harness

#### Connector Part Information

- OEM: 7283-6443-40
- Service: See Catalog
- Description: 2-Way F 1.5 YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-6443-40
- Service: See Catalog
- Description: 2-Way M 1.5 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X911 Liftgate Harness to Center High Mounted Stop Lamp (CHMSL) Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BK | 650 | Ground | 1 | 0.5 BK | 650 | Ground
2 | 0.5 L-BU | 1320 | Stop Lamp Voltage | 2 | 0.5 L-BU | 1320 | Stop Lamp Voltage

### X920 Liftgate Harness to Liftgate Applique Harness (W49 or Z88)

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177532
- Service: 15306377
- Description: 3-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X920 Liftgate Harness to Liftgate Applique Harness (W49 or Z88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Voltage | A | 0.5 BK | -- | Backup Lamp Voltage (Z88)
0.5 WH | -- | Backup Lamp Voltage (W49)
B | 0.5 PU | 709 | Left Park Lamp Voltage | B | 0.5 BK | -- | Left Park Lamp Voltage (Z88)
0.5 BN | -- | Left Park Lamp Voltage (W49)
C | 0.5 BK | 650 | Ground | C | 0.5 BK | -- | Ground

### X931 Liftgate Harness to Liftgate Applique Harness (W49 or Z88)

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 19177532
- Service: 15306377
- Description: 3-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X931 Liftgate Harness to Liftgate Applique Harness (W49 or Z88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Voltage | A | 0.5 BK | -- | Backup Lamp Voltage (Z88)
0.5 WH | -- | Backup Lamp Voltage (W49)
B | 0.5 PU | 709 | Left Park Lamp Voltage | B | 0.5 BK | -- | Left Park Lamp Voltage (Z88)
0.5 BN | -- | Left Park Lamp Voltage (W49)
C | 0.5 BK | 650 | Ground | C | 0.5 BK | -- | Ground

### X933 License Lamp Harness to Liftgate Harness (without X88)

#### Connector Part Information

- OEM: 7283-7696-40
- Service: See Catalog
- Description: 12-Way F YESC Kaizen Series (L-GY)

#### Connector Part Information

- OEM: 7282-7696-40
- Service: See Catalog
- Description: 12-Way M YESC Kaizen Series, Unsealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X933 License Lamp Harness to Liftgate Harness (without X88)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 PK | 6972 | Camera Video Signal (+) (UVC) | 1 | 0.35 PK | 6972 | Camera Video Signal (+) (UVC)
2 | 0.35 BARE | 6974 | Camera Shield (UVC) | 2 | 0.35 BARE | 6974 | Camera Shield (UVC)
3 | 0.35 GY | 5797 | Liftgate Open/Close Switch Signal Rear (TB4) | 3 | 0.35 GY | 5797 | Liftgate Open/Close Switch Signal Rear (TB4)
0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal (TB5) | 0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal (TB5)
4 | 0.5 BK | 709 | Left Park Lamp Voltage | 4 | 0.5 PU | 709 | Left Park Lamp Voltage
5 | 0.5 WH | 650 | Ground | 5 | 0.5 BK | 650 | Ground
6 | 0.35 L-BU | 6973 | Camera Video Signal (-) (UVC) | 6 | 0.35 L-BU | 6973 | Camera Video Signal (-) (UVC)
7 | 0.35 BK | 650 | Ground (TB4) | 7 | 0.35 BK | 650 | Ground (TB4)
0.35 PU/WH | 5801 | Low Reference (TB5) | 0.35 PU/WH | 5801 | Low Reference (TB5)
8 | 0.35 PK | 239 | Ignition Voltage (UVC) | 8 | 0.35 PK | 239 | Ignition Voltage (UVC)
9 | 0.35 BK | 650 | Ground (UVC) | 9 | 0.35 BK | 650 | Ground (UVC)
10 | 0.35 D-BU | 38 | Backup Lamp Relay Control (UVC) | 10 | 0.35 D-BU | 38 | Backup Lamp Relay Control (UVC)
11-12 | -- | -- | Not Used | 11-12 | -- | -- | Not Used

### X940 Liftgate Harness to Liftgate Trim Panel Harness

#### Connector Part Information

- OEM: 7283-3440-40
- Service: 19149536
- Description: 3-Way F Kaizen YESC Series (L-GY)

#### Connector Part Information

- OEM: 7282-3440-40
- Service: See Catalog
- Description: 3-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4101-08/9
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X940 Liftgate Harness to Liftgate Trim Panel Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 GY/BK | 690 | Courtesy Lamp High Control | 1 | 0.5 GY/BK | 690 | Courtesy Lamp High Control
1 GY/BK | 690 | Courtesy Lamp High Control
2 | 1 BK | 650 | Ground | 2 | 0.5 BK | 650 | Ground
1 BK | 650 | Ground
3 | -- | -- | Not Used | 3 | -- | -- | Not Used