For 1990-2009 cars

## Rear Seat Adjuster Handle Replacement With 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the outer rear seat cushion trim panel. Refer to Rear Seat Cushion Trim Panel Assembly Replacement - Outboard or Rear Seat Cushion Trim Panel Assembly Replacement - Inboard.
3. Remove the rear seat recliner outer finish covers. Refer to Rear Seat Recliner Outer Finish Cover Replacement - Inboard or Rear Seat Recliner Outer Finish Cover Replacement - Outboard.

1 | Rear Seat Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | Rear Seat Adjuster Handle Assembly

#### Procedure

Disconnect the cables at the inboard and outboard recliners.

## Rear Seat Adjuster Handle Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the outer rear seat cushion trim panel assembly. Refer to Rear Seat Cushion Trim Panel Assembly Replacement - Outboard or Rear Seat Cushion Trim Panel Assembly Replacement - Inboard.
3. Remove the rear seat recliner outer finish covers. Refer to Rear Seat Recliner Outer Finish Cover Replacement - Inboard or Rear Seat Recliner Outer Finish Cover Replacement - Outboard.

1 | Rear Seat Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | Rear Seat Adjuster Handle Assembly

#### Procedure

Disconnect the cables at the inboard and outboard recliners.