For 1990-2009 cars

## Rear Seat Number 2 Belt Buckle Replacement With 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove third row seat. Refer to Rear Number 2 Seat Replacement.
2. Remove rear storage compartment. Refer to Rear Storage Compartment Replacement.

1 | Rear Seat No.2 (Buckle Side) Belt and Bolt Assembly Caution: Refer to Fastener Caution in the Preface section. Tighten 53 N·m (39 lb ft)

## Rear Seat Number 2 Belt Buckle Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove third row seat. Refer to Rear Number 2 Seat Replacement.
2. Remove rear storage compartment if equipped. Refer to Rear Storage Compartment Replacement.

1 | Rear Seat No.2 (Buckle Side) Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 53 N·m (39 lb ft)
2 | Rear Seat No.2 (Buckle Side) Belt Assembly
3 | Rear Seat No.2 Center (Buckle Side) Belt Assembly Tighten 53 N·m (39 lb ft)