For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat No. 2 back cushion panel. Refer to Rear Seat Number 2 Back Cushion Panel Replacement .
2. Remove the rear seat No. 2 head restraint. Refer to Rear Seat Number 2 Head Restraint Replacement .

1 | Rear Seat No. 2 Cushion Cover

#### Procedure

1. Disconnect the j-channel from the seat back cushion frame.
2. Remove the seat back cushion cover from pad.
3. Remove the swing wire between the inner and outer pads.
4. Remove the seat back cushion cover from the pad.

2 | Rear Seat No. 2 Back Cushion Pad