For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the left catalytic convertor. Refer to Catalytic Converter Replacement - Left Side.
3. Remove the starter heat shield bolt and shield.
4. Remove the starter solenoid BAT terminal nut (3).
5. Remove the battery positive junction block cable terminal (2) from the starter.
6. Disconnect the engine wiring harness electrical connector (1) from the starter.
7. Remove the starter bolts and starter.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the starter and bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

2. Connect the engine wiring harness electrical connector (1) to the starter.
3. Install the battery positive junction block cable terminal (2) to the starter.
4. Install the starter solenoid BAT terminal nut (3).

Tighten
Tighten the nut to 25 N·m (18 lb ft).

5. Install the starter heat shield and bolt.

Tighten
Tighten the bolt to 7 N·m (62 lb in).

6. Install the left catalytic convertor. Refer to Catalytic Converter Replacement - Left Side.
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.