For 1990-2009 cars

### Description

Point-to-point measurements are for reference only. All measurements are given im millimeters. Use these measurements for diagnosing and estimating. Point-to-point measurements are duplicated with tram bar pointers set at equal lengths. All die marks, holes, slots, and fasteners are measured to the center. All dimensions are symetrical unless otherwise specified.

### Underhood Opening Dimensions

### Body Side Opening Dimensions

### Rear Body Opening Dimensions