For 1990-2009 cars

# Engine

## All Description and Operation

- Cooling Fan Description and Operation
- Cooling System Description and Operation

## All Special Tools and Equipment

- Special Tools

## Cleaning, Inspection, and Adjustment

- Cooling System Draining and Filling
- Flushing
- Radiator Cleaning

## Diagnostic Procedures

- Coolant Heater Inoperative
- Cooling Fan Always On
- Cooling Fan Inoperative
- Cooling System Leak Testing
- Diagnostic Starting Point - Engine Cooling
- Engine Fails To Reach Normal Operating Temperature
- Engine Overheating
- Loss of Coolant
- Pressure Cap Testing
- Symptoms - Engine Cooling
- Thermostat Diagnosis

## Diagnostic Trouble Codes

- DTC P0480, P0481, P0691, P0692, P0693, or P0694
- DTC P1258

## Electrical/Electronic Schematic Diagrams

- Engine Cooling Schematics

## Mechanical Specifications

- Fastener Tightening Specifications

## Removal, Installation, and Replacement

- Coolant Heater Cord Replacement
- Coolant Heater Replacement
- Coolant Recovery Reservoir Replacement
- Cooling Fan and Shroud Replacement
- Engine Coolant Thermostat Replacement
- Engine Oil Cooler Connector Replacement
- Engine Oil Cooler Hose/Pipe Quick-Connect Fitting Disconnection and Connection
- Radiator Inlet Hose Replacement
- Radiator Outlet Hose Replacement
- Radiator Replacement
- Water Outlet Replacement
- Water Pump Replacement