For 1990-2009 cars

Checks | Causes
--- | ---
Fluid Pump Assembly (203) |

• | Inspect for loose Fluid Pump Bolts (204)

• | Inspect for leaking or damaged Fluid Pump Outlet Seals (57) and Oil Filter Seal (202)

• | Inspect for improperly installed or damaged Oil Filter (201)

• | Inspect for sticking Line Pressure Blow Off Valve

Front Differential Drive Gear Support Assembly (208) |

• | Inspect for leaking or damaged Drive Gear Support Torque Converter Seal Assembly (206) or Fluid Passage Tube Gasket (212)

• | Inspect for leaking or damaged Drive Gear Support Fluid Passage Tube Assembly (209)

Upper Valve Body Assembly (312) |

• | Inspect for leaking or damaged Upper Valve Body Assembly (309) Gasket

• | Inspect for worn, sticking or damaged Pressure Regulator Valve (337) or Pressure Regulator Valve Spring (338)

Lower Valve Body Assembly (313) | Inspect for leaking or damaged Lower Valve Body Assembly (313) Gasket
Control Valve (w/Body & TCM) Valve Assembly (15) | Inspect for leaking or damaged Filter Plate Assembly Seals (16)
Case Assembly (51) | Inspect for missing Lube Oil Circuit Orifice or Baffle (229)