For 1990-2009 cars

## Parking and Turn Signal Lamp Bracket Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the main electrical harness connector at the park and front fog lamp bracket assembly.

1 | Front Bumper Fascia Brace Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Park and Front Fog Lamp Bracket Screw (Qty: 2) Tighten 2 N·m (18 lb in)
3 | Park and Front Fog Lamp Bracket

#### Procedure

1. Remove the bracket assembly from the front end upper tie bar support.
2. Remove and transfer the park turn signal lamp assembly. Refer to Parking and Turn Signal Lamp Replacement.
3. Remove and transfer the fog lamp assembly, if equipped. Refer to Front Fog Lamp Replacement.
4. Remove and transfer the electrical jumper harness.