For 1990-2009 cars

Checks | Causes
--- | ---
Low and Reverse Clutch Assembly (455) |

• | Inspect for disengaged or broken Low and Reverse Clutch Retainer (454)

• | Inspect for stripped or sheared splines on Low and Reverse Clutch (455)

Low and Reverse Clutch |

• | Inspect for stripped or sheared splines on Low and Reverse Clutch Plates (449-453)

• | Inspect for damaged, deformed or improper surface finish on the Low and Reverse Clutch Plates (449-453)

Case Cover Assembly (403) |

• | Inspect for disengaged or broken Low and Reverse Clutch Piston Spring Retainer (410)

• | Inspect for worn, damaged or debonding Low and Reverse Clutch Piston Seals (408)

• | Inspect for broken or deformed Low and Reverse Clutch Piston (408)

• | Inspect for improperly position or too large bleed hole in Low and Reverse Piston (408)

• | Inspect for porosity or improper finish on the Case Cover