For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Wiring Junction Block Nut | 22 N·m | 16 lb ft
Air Conditioning Liquid Line Clamp Bolt | 9 N·m | 80 lb in
Battery Cover Screw | 1.6 N·m | 14 lb in
Battery Hold Down Bolt | 25 N·m | 18 lb ft
Battery Negative Cable Extension Cable to Cylinder Head Bolt | 58 N·m | 43 lb ft
Battery Negative Cable Extension Cable to Left Wheelhouse Panel Upper Reinforcement Bolt | 58 N·m | 43 lb ft
Battery Positive Junction Block Cable to Generator Nut | 22 N·m | 16 lb ft
Coolant Recovery Reservoir Bolt | 5 N·m | 44 lb in
Generator Bolt | 50 N·m | 37 lb ft
Negative Battery Cable Ground Bolt | 25 N·m | 18 lb ft
Negative Battery Cable Terminal Nut | 9 N·m | 80 lb in
Positive Battery Cable Terminal Nut | 9 N·m | 80 lb in
Starter Bolt | 50 N·m | 37 lb ft
Starter Heat Shield Bolt | 7 N·m | 62 lb in
Starter Solenoid BAT Terminal Nut | 25 N·m | 18 lb ft