For 1990-2009 cars

## Rear Seat Back Cushion Latch Release Handle Replacement with 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Latch Release Handle Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Seat Latch Release Handle Assembly

#### Procedure

• | Disconnect the cable and note the cable routing for installation.

• | The cable must be routed under the rear seat back stowage latch housing.

• | The white area of the cable must fit into the seat back frame hooks.

## Rear Seat Back Cushion Latch Release Handle Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Back Cushion Latch Release Handle Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Seat Back Cushion Latch Release Handle Assembly

#### Procedure

• | Disconnect the cable and note the cable routing for installation.

• | The cable must be routed under the rear seat back stowage latch housing.

• | The white area of the cable must fit into the seat back frame hooks.