For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the inner window belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement.
3. Remove the outer window belt sealing strip. Refer to Rear Side Door Window Outer Sealing Strip Replacement.
4. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
5. Remove the window. Refer to Rear Side Door Window Replacement.

1 | Rear Side Door Stationary Window Upper Screws (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip The quarter glass and weatherstrip/run channel is not serviceable and should be replaced only as an assembly. Tighten
5 N·m (44 lb in)

2 | Rear Side Door Stationary Window Bolt Tighten 10 N·m (89 lb in)
3 | Rear Side Door Stationary Window Bolts (Qty: 2) Tighten 10 N·m (89 lb in)
4 | Rear Side Door Stationary Window

#### Procedure

1. When removing carefully twist the weatherstrip run channel and pull up at the top of the door frame.
2. Press the weatherstrip/run channel into the window frame opening.
3. Position the tabs on the weatherstrip/run channel into the slots on the door.
4. Attach the molding to the outside of the door with double sided tape.