For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat. Refer to Bucket Seat Replacement.
2. Remove the front seat front finish cover. Refer to Front Seat Front Finish Panel Replacement.

1 | Front Seat Adjuster Finish Cover Bracket Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | Front Seat Adjuster Finish Cover Bracket