For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the window. Refer to Front Side Door Window Replacement.
4. Remove the door speaker. Refer to Radio Front Side Door Speaker Replacement.
5. Remove the 2 bolts (1) that retain the weatherstrip/run channel (2) to the door.
6. Pull the weatherstrip/run channel away from the window frame opening.
7. Carefully twist and pull up on the weatherstrip/run channel, in order remove the weatherstrip/run channel from the top of the door frame.
8. Remove the weatherstrip/run channel from the door.

### Installation Procedure

1. Install the weatherstrip/run channel (2) to the door.
2. Position the tabs on the weatherstrip/run channel into the slots in the door.
3. Press the weatherstrip/run channel into the window frame opening.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the retaining bolts (1).

Tighten
Tighten the retaining bolts to 10 N·m (88 lb in).

5. Install the door speaker. Refer to Radio Front Side Door Speaker Replacement.
6. Install the window. Refer to Front Side Door Window Replacement.
7. Install the water deflector. Refer to Front Side Door Water Deflector Replacement.
8. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side.