For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: After cleaning the transmission components, allow to air dry. Do not use cloth or paper towels in order to dry any transmission components. Lint from the towels can cause component failure. Caution: Do not reuse cleaning solvents. Previously used solvents may deposit sediment which may damage the component.

#### Preliminary Procedure

The fluid pump assembly is not serviceable.

1 | Filter Neck Seal Tip Install a NEW filter neck seal.

#### Special Tools

28585 Snap ring Remover or equivalent

For equivalent regional tools, refer to Special Tools.

2 | A/Trans Fluid Filter Assembly Tip Install a NEW fluid filter assembly.
3 | Fluid Pump Drive Shaft Tip

• | Inspect the fluid pump drive shaft splines for damage or wear.

• | Rotate the fluid pump drive shaft for free operation.