For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. It is only necessary to lower the headliner. Only do those steps in the headliner replacement procedure that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement.
2. Remove the sunroof module. Refer to Sunroof Frame Replacement

1 | Sunroof Sunshade Trim Cover Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Sunroof Sunshade Trim Cover Retainer (Qty: 2)
3 | Sunroof Sunshade Trim Cover Screw (Qty: 6) Tighten 2 N·m (18 lb in)
4 | Sunroof Sunshade Trim Cover Tip The sunroof sunshade trim cover is separate from the module.