For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the underbody rear side rail. Refer to Underbody Rear Side Rail Replacement.
3. Support the frame with a jack stand.

1 | Frame Reinforcement Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 60 N·m (44 lb ft)
2 | Frame Reinforcement Stud Tighten 60 N·m (44 lb ft)
3 | Frame Bolt (Qty: 2) Tighten 110 N·m (81 lb ft) plus 90 degrees
4 | Frame Reinforcement (Qty: 2)