For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side.

1 | Outside Rearview Mirror Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
10 N·m (89 lb in)

2 | Outside Rearview Mirror

#### Procedure

Remove the retainer holding the window reveal molding at the lower corner of the door in three positions.