For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.

1 | Front Seat Lumbar Control Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Front Seat Lumbar Control

#### Procedure

Disconnect the lumbar cable from the control assembly for removal.