For 1990-2009 cars

## Hood Front Molding Replacement Acadia

Callout | Component Name
--- | ---
1 | Hood Molding Integral Retainer Tab (Qty 3)
2 | Hood Front Molding Tip Release the 3 integral retainers from the front edge of the hood.

## Hood Front Molding Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the hood.

1 | Front Hood Molding

#### Procedure

1. Carefully release the 6 integral retainers securing the molding to the front edge of the hood.
2. Upon installation, align the center pin first to the hood and work outward securing the integral retainers to the hood.

2 | Hood Front Molding