For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear tire and wheel. Refer to Tire and Wheel Removal and Installation .
3. Position an adjustable jack stand under the lower control arm .
4. Remove the lower stabilizer shaft link bushing and nut. Refer to Stabilizer Shaft Link Replacement .
5. Remove the lower shock absorber bolt. Refer to Shock Absorber Replacement .
6. Remove the lower bolts from the knuckle. Refer to Knuckle Replacement .
7. Using the adjustable jack stand, slowly lower the vehicle until the rear spring (1), insulator (4), jounce bumper (2), and the spring seat (3) can be removed.

### Installation Procedure

1. Position the spring seat (3), jounce bumper (2), rear spring (1), and the insulator (4) on the lower control arm.
2. Using the adjustable jack stand, raise the lower control arm until the lower bolts for the knuckle can be installed. Refer to Knuckle Replacement .
3. Remove the adjustable jack stand.
4. Install the lower stabilizer shaft link bushing and nut. Refer to Stabilizer Shaft Link Replacement .
5. Install the lower shock absorber bolt. Refer to Shock Absorber Replacement .
6. Install the rear tire and wheels. Refer to Tire and Wheel Removal and Installation .
7. Remove the support and lower the vehicle.