For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the center pillar lower garnish molding. Refer to Center Pillar Lower Garnish Molding Replacement.

1 | Center Pillar Upper Garnish Molding Screw Caution: Refer to Fastener Caution in the Preface section. Tip Open the access door to remove the screw. Tighten
2 N·m (18 lb in)

2 | Center Pillar Upper Garnish Molding Assembly

#### Procedure

Route the seat belt through the molding prior to installing.