For 1990-2009 cars

### Removal Procedure

1. Remove the front door sill plate. Refer to Front Side Door Sill Plate Replacement .
2. Remove the weatherstrip (1) from the pinch-weld flange (2).

### Installation Procedure

1. Align the weatherstrip to the door opening with the bond joint positioned at the lower center of the door opening.
2. Install the weatherstrip to the pinch-weld flange. Ensure the weatherstrip is fully seated.
3. Install the front door sill plate. Refer to Front Side Door Sill Plate Replacement .