For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Lock Pin Warning: Lock pin must be secured into the bench fixture to hold the transmission and prevent bodily injury. Tip Ensure the J 3289-20 holding fixture is mounted to a bench that is properly supported and will support the weight of the transmission assembly without tipping. J-39890 holding fixture adapter adapter and an engine stand can be used as an alternative method for supporting the transmission assembly during repairs.

#### Special Tools

• | J 3289-20 Holding Fixture

• | J-39890 Transmission Holding Fixture Adapter

For equivalent regional tools, refer to Special Tools.

2 | J 21366 Converter Holding Strap For equivalent regional tools, refer to Special Tools.
3 | Dust Cover Bolts M10 x 25, model dependent (Qty: 2)
4 | Dust Cover Push Pin, model dependant
5 | Dust Cover, model dependant
6 | Torque Converter Assembly Caution: Only install the lift assist handles until it stops. Do not tighten. Over tightening the lift assist handles can cause damage to the torque converter. Tip Failure to raise the torque converter straight up could damage the torque converter clutch lip seal inside the torque converter clutch assembly.

#### Special Tools

J 46409 Torque Converter Lifting Handles

For equivalent regional tools, refer to Special Tools.