For 1990-2009 cars

## Rear Seat Frame Front Finish Cover Replacement - Lower with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Frame Front Finish Cover (Qty: 2)

#### Procedure

1. Pull outward at the rear edge of the cover to disengage the rear retainer clip.
2. Pull the front inner corner of the cover inward to disengage the cover from the seat cushion frame.
3. Pull forward to disengage the remaining retainer clip from the front edge of the cover.

2 | Retainer Clip (Qty: 6)

## Rear Seat Frame Front Finish Cover Replacement - Lower with 60 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Frame Front Finish Cover (Qty: 2)

#### Procedure

1. Pull outward at the rear edge of the cover to disengage the rear retainer clip.
2. Pull the front inner corner of the cover inward to disengage the cover from the seat cushion frame.
3. Pull forward to disengage the remaining retainer clip from the front edge of the cover.

2 | Retainer Clip (Qty: 6)