For 1990-2009 cars

## Rear Seat Back Cushion Panel Replacement with 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Back Cushion Panel Tip Squeeze the retainers from the front side of the seat back and push rearward to disengage from the seat back frame.

## Rear Seat Back Cushion Panel Replacement with 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Back Cushion Panel Tip Squeeze the retainers from the front side of the seat back and push rearward to disengage from the seat back frame.