For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Link to Knuckle Nut

- First Pass

75 N·m

55 lb ft

- Final Pass

+ 60 degrees

Adjuster Link to Crossmember Nuts | 140 N·m | 103 lb ft
Lower Control Arm to Knuckle Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

+ 60 degrees

Lower Control Arm to Crossmember Nuts - Front

- First Pass

110 N·m

81 lb ft

- Final Pass

+ 45 degrees

Lower Control Arm to Crossmember Nuts - Rear

- First Pass

120 N·m

89 lb ft

- Final Pass

+ 60 degrees

Upper Rear Shock Absorber Nuts | 70 N·m | 52 lb ft
Rear Shock Absorber to Lower Control Arm Bolts

- First Pass

100 N·m

74 lb ft

- Final Pass

+ 60 degrees

Rear Wheel Bearing and Hub to Knuckle Bolts | 140 N·m | 103 lb ft
Stabilizer Shaft Clamp to Crossmember Bolts | 50 N·m | 37 lb ft
Stabilizer Shaft Link Nuts | 22 N·m | 16 lb ft
Upper Control Arm to Knuckle Bolts

- First Pass

100 N·m

74 lb ft

- Final Pass

+ 90 degrees

Upper Control Arm to Crossmember Nuts | 140 N·m | 103 lb ft
Wheel Drive Shaft Nut | 205 N·m | 151 lb ft