For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When performing service on or near the SIR components or the SIR wiring, the SIR system must be disabled. Refer to SIR Disabling and Enabling . Failure to observe the correct procedure could cause deployment of the SIR components, personal injury, or unnecessary SIR system repairs.

Warning: Do not strike or jolt the inflatable restraint side impact sensor (SIS). Before applying power to the SIS make sure that it is securely fastened. Failure to observe the correct installation procedures could cause SIR deployment, personal injury, or unnecessary SIR system repairs.

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Remove front side door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side.
3. Remove front side door water deflector. Refer to Front Side Door Water Deflector Replacement.

1 | Inflatable Restraint Side Impact Sensor Module Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Loosen the bolts and slide sensor out of key hole slots.
2. Disconnect the electrical connector.

Tighten
9 N·m (80 lb in)

2 | Inflatable Restraint Side Impact Sensor Module