For 1990-2009 cars

Checks | Causes
--- | ---
Input Carrier Assemlby (470) | Inspect for worn or stripped Ring Gear Splines
Case Assembly (51) |

• | Inspect for damaged or fatigued 1-2-3-4 Clutch Wave Plate (458) and Low & Reverse Clutch Wave Plate (450)

• | Inspect for stripped or worn splines on 1-2-3-4 Clutch Plate (456)

• | Inspect for improperly positioned or plugged Low Reverse Piston (408) air bleed

• | Inspect for correct fluid level