For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Sight Shield Push Pin (Qty: 8)
2 | Sight Shield
3 | Hood Latch Mounting Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
4 | Hood Latch Assembly
5 | Hood Release Cable

#### Procedure

1. Disconnect the remote start electrical connector, if equipped.
2. Disconnect the release cable from the hood latch by squeezing the cable retainer.