For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Bucket Seat Replacement .

1 | Front Seat Back Cushion Rear Finish Panel

#### Procedure

1. Using a flat bladed tool, from the side, push inward on the top two retainers while pulling rearward at the top of the panel.
2. Lift the panel upward to remove from the seat.

2 | Front Seat Head Restraint Assembly

#### Procedure

1. Push the button on the outer head restraint guide in to adjust the head restraint to the highest position.
2. Push the button on the inner head restraint guide in while pulling upward to finish releasing the head restraint from the seat.

3 | Front Seat Head Restraint Guide (Qty: 2) Tip Use a rubber mallet or equivalent to tap upward on the bottom of the head restraint guide to remove from the seat back frame.
4 | Front Seat Back Cushion Cover

#### Procedure

1. Disengage the j-channel retainers from the seat back cushion frame.
2. Disconnect the electrical connectors that attach to the seat back cushion, if equipped.
3. Loosen the inflatable restraint side impact module nuts.
4. Slide the inflatable restraint side impact module out of the sleeve. Refer to Driver and Passenger Seat Side Inflatable Restraint Module Replacement .
5. Remove the seat back cushion cover and pad as an assembly.
6. Remove the hog rings in order to pull the cover away from the pad.

5 | Front Seat Back Cushion Pad