For 1990-2009 cars

## Rear Side Door Trim Panel Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear door upper extension trim panel. Refer to Upper Extension Trim Panel Replacement.

1 | Rear Side Door Pull Handle Cover Tip Install the top portion of the pull handle cover first to ensure tabs are lined up and push the cover in firmly.
2 | Rear Side Door Inside Handle Bezel Finish Cover
3 | Rear Side Door Trim Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
4 | Rear Side Door Locking Rod Knob Assembly

#### Procedure

1. Ensure the locking rod is in the unlocked position.
2. Use a flat-bladed tool to disengage the detent tab and then remove the knob by pulling upward.
3. When re-installing, push the knob down until the detent tab touches the locking rod opening cover.
4. Push the detent tab into the lock knob to locking rod.

5 | Rear Side Door Trim Panel Retainer (Qty: 9)
6 | Rear Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the 9 retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

## Rear Side Door Trim Panel Replacement Acadia/OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear door upper extension trim panel. Refer to Upper Extension Trim Panel Replacement.

1 | Rear Side Door Pull Handle Cover Tip Install the top portion of the pull handle cover first to ensure tabs are lined up and push the cover in firmly.
2 | Rear Side Door Inside Handle Bezel Finish Cover
3 | Rear Side Door Trim Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
4 | Rear Side Door Locking Rod Knob Assembly

#### Procedure

1. Ensure the locking rod is in the unlocked position.
2. Use a flat-bladed tool to disengage the detent tab and then remove the knob by pulling upward.
3. When re-installing, push the knob down until the detent tab touches the locking rod opening cover.
4. Push the detent tab into the lock knob to locking rod.

5 | Rear Side Door Trim Panel Retainer (Qty: 9)
6 | Rear Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the 9 retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

## Rear Side Door Trim Panel Replacement Enclave

Callout | Component Name
--- | ---
1 | Rear Side Door Pull Handle Cover
2 | Rear Side Door Inside Handle Bezel Finish Cover
3 | Rear Side Door Trim Panel Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (18 lb in)
4 | Rear Side Door Trim Panel Assembly

#### Procedure

1. Use a door trim pad removal tool, or equivalent, at each of the 9 retainer locations to aid in the removal of the trim panel.
2. Disengage the door lock cable.
3. Disconnect the electrical connector.

5 | Rear Side Door Trim Panel Retainer (Qty: 9)