For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Latch Release Handle Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Seat Back Latch Release Strap Bezel