For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the canister purge tube quick connect fittings from the purge solenoid. Refer to Plastic Collar Quick Connect Fitting Service.

1 | Evaporative Emission Canister Purge Solenoid Valve Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Evaporative Emission Canister Purge Solenoid Valve

#### Procedure

Disconnect the electrical connector.