For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Side Door Window Front Channel Bolt Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Remove the lower section of the channel weatherstrip from the channel.

Tighten
10 N·m (89 lb in)

2 | Rear Side Door Window Front Channel

#### Procedure

1. Remove the front door weatherstrip channel by pulling downward to release it from the upper door frame.
2. When installing the channel ensure that the lower channel aligns with the upper channel before install the channel weatherstrip.
3. Verify that the window work properly in the channel weatherstrip.

3 | Rear Side Door Window Rear Channel Bolt Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Remove the lower section of the channel weatherstrip from the channel.

Tighten
10 N·m (89 lb in)

4 | Rear Side Door Window Rear Channel

#### Procedure

1. Remove the rear door weatherstrip channel by pulling downward to release it from the upper door rear frame.
2. When installing the channel ensure that the lower channel aligns with the upper channel before install the channel weatherstrip.
3. Verify that the window work properly in the channel weatherstrip.