For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the I/P trim pad. Refer to Instrument Panel Trim Pad Replacement.

1 | Right Side Window Defogger Outlet Duct Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Right Side Window Defogger Outlet Duct

#### Procedure

Squeeze tab to release from windshield defroster duct.