For 1990-2009 cars

#### Special Tools

• | EN-48253 Accessory Belt Remover

• | EN-48952 Tensioner Spring Holding Pin

### Removal Procedure

1. Remove the front compartment insulator. Refer to Front Compartment Insulator Replacement.
2. Install the EN-48253 remover (3) onto the tensioner and rotate the drive belt tensioner clockwise.
3. Rotate the drive belt tensioner fully and simultaneously insert EN-48952 holder (2) into the drive belt tensioner pin hole.
4. Remove the drive belt (4).

### Installation Procedure

1. Install the drive belt.
2. Install the EN-48253 remover (3).
3. Rotate the drive belt tensioner (1) clockwise fully and simultaneously remove EN-48952 holder (2) out of the drive belt tensioner pin hole.
4. Install the front compartment insulator. Refer to Front Compartment Insulator Replacement.