For 1990-2009 cars

#### Special Tools

• | EN-48253 Accessory Belt Remover

• | EN-48952 Tensioner Spring Holding Pin

| For equivalent regional tools, refer to Special Tools.

1. Install the generator and air conditioning compressor and power steering pump belt.
2. Install the EN-48253 remover .
3. Rotate the drive belt tensioner (1) clockwise fully and simultaneously remove EN-48952 holder (2) out of the drive belt tensioner pin hole.