For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the wheel drive shaft. Refer to Front Wheel Drive Shaft Replacement - Right Side.

1 | Front Wheel Drive Intermediate Shaft Bracket Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tip Use care when removing the intermediate drive shaft from the transmission as not to damage the seal. Tighten
9 N·m (80 lb ft)

2 | Front Wheel Drive Intermediate Shaft Tip The DT-6332 protector must be installed into the differential output shaft seal prior to removing and installing the intermediate shaft. Failure to install the DT-6332 protector may cause splines of the intermediate shaft to cut the differential output seal.

#### Special Tools

DT-6332 Seal Protector

For equivalent regional tools, refer to Special Tools.