For 1990-2009 cars

NEED GRAPHIC

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove front side door trim. Refer to Front Side Door Trim Replacement.
2. Remove front side door window switch bezel. Refer to Front Side Door Window Switch Bezel Replacement.

1 | Side Window Switch Bezel
2 | Power Mirror Switch

#### Procedure

1. Using a plastic pry tool, gently pry on the sides to release the switch.
2. Disconnect the electrical connector.