For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear side door trim panel. Refer to Rear Side Door Trim Replacement.

1 | Rear Side Door Check Link Bolt Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Disconnect the door electrical connector.
3. Support the door before removing the hinge bolts.
4. With the aid of an assistant, remove the door.

Tighten
25 N·m(18 lb ft)

2 | Rear Side Door Lower Hinge Bolt (Qty: 2) Tighten 25 N·m(18 lb ft)
3 | Rear Side Door Upper Hinge Bolt (Qty: 2) Tighten 25 N·m(18 lb ft)
4 | Rear Side Door

#### Procedure

1. Transfer all of the internal components.
2. Adjust the rear side door as needed. Refer to Rear Door Adjustment.