For 1990-2009 cars

## Exhaust Particulate Filter Replacement 2.0L Diesel LLW

Callout | Component Name
--- | ---
Warning: Refer to Exhaust Service Warning in the Preface section. Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front compartment insulator. Refer to Front Compartment Insulator Replacement.

1 | Exhaust Pressure Differential Sensor Hose Clamp (Qty: 2)
2 | Exhaust Pressure Differential Sensor Hose (Qty: 2) Note: Different diameters consider.
3 | Rear Exhaust Temperature Sensor Wiring Harness Plug
4 | Exhaust Flex Pipe to Exhaust Particulate Filter Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 40 N·m (30 lb ft)
5 | Exhaust Particulate Filter Nut (Qty: 2) Tighten 40 N·m (30 lb ft)
6 | Exhaust Particulate Filter Hanger Bracket Bolt (Qty: 2) Tighten 17 N·m (13 lb ft)
7 | Exhaust Particulate Filter