For 1990-2009 cars

## Clutch Actuator Cylinder Pipe Replacement D16

### Removal Procedure

1. Remove the manual transmission. Refer to Transmission Replacement.
2. Remove the clutch actuator cylinder pipe connector (1) from the clutch housing.
3. Remove the clutch actuator cylinder pipe (2).

### Installation Procedure

1. Install the clutch actuator cylinder pipe connector (1) to the clutch housing.
2. Install the clutch actuator cylinder pipe (2).
3. Install the manual transmission. Refer to Transmission Replacement.

## Clutch Actuator Cylinder Pipe Replacement D33

### Removal Procedure

1. Remove the manual transmission. Refer to Transmission Replacement.
2. Remove the clutch actuator cylinder pipe connector (1) from the clutch housing.
3. Remove the clutch actuator cylinder pipe (2).

### Installation Procedure

1. Install the clutch actuator cylinder pipe connector (1) to the clutch housing.
2. Install the clutch actuator cylinder pipe (2).
3. Install the manual transmission. Refer to Transmission Replacement.