For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the hood insulator. Refer to Hood Insulator Replacement.
2. Place a clean container under the front driver side near where the windshield washer nozzle and windshield washer pump hose will be disconnected.
3. Recover all lost windshield washer solvent.

1 | Windshield Washer Nozzle Hose Tip Disconnect the washer hose from both hood mounted washer nozzles.
2 | Windshield Washer Hose Retainer to Hood Hinge
3 | Windshield Washer Nozzle Hose Integral Connector Tip Disconnect the hoses in order to remove the windshield washer nozzle hose.
4 | Windshield Washer Pump Hose