For 1990-2009 cars

Caution: Refer to Fastener Caution in the Preface section.

1. Install the electronic throttle actuator control module gasket (4)
2. Install the electronic throttle actuator control module (1).
3. Install the wiring harness plug (2).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 2 electronic throttle actuator control module nuts (2) and tighten to 9 N·m (80 lb in).
5. Install the 2 electronic throttle actuator control module bolts (3) and tighten to 9 N·m (80 lb in).
6. Install the wiring harness plug (2) at the electronic throttle actuator control module (1).