For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the intake air duct bolt (2).
3. Remove the intake air duct (1).

### Installation Procedure

1. Install the intake air duct (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the intake air duct bolt (2) and tighten the bolt to 5 Nm (45 lb in).
3. Install the front bumper facia. Refer to Front Bumper Fascia Replacement.