For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
2. Disconnect the front turn signal lamp electrical connector from the forward lamp harness assembly at the topside of the fender panel.
3. Rotate the lamp socket from the lamp housing.
4. Squeeze the lamp housing locking tab and push outward in order to remove the lamp housing from the fender panel.

1 | Front Turn Signal Lamp Assembly

#### Procedure

Replace the bulb, as needed.