For 1990-2009 cars

Caution: The steering column must be in the LOCK position before disconnecting the following components:

• | The steering column

• | The steering shaft coupling

• | The intermediate shaft

• | The lower steering shaft

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.

### Removal Procedure

1. Turn the steering wheel to the straight forward position and support it from movement.
2. Remove the 2 intermediate steering shaft bolts.
3. Remove the intermediate steering shaft.

### Installation Procedure

1. Install the intermediate steering shaft.

Note: The recess (2) of the fine toothing in the universal joint have to align precisely with the recess (1) of the fine toothing on the steering pinion. The bore in the universal joint have to align with the groove on the steering pinion (3).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 intermediate steering shaft bolts. Tighten the intermediate steering shaft bolts XX N·m (XX lb ft).