For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
2. Remove the front fender insulator. Refer to Front Fender Insulator Replacement.
3. Remove the front side door. Refer to Front Side Door Replacement.

1 | Front Side Door Hinge Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m(19 lb ft)
2 | Front Side Door Hinge

#### Procedure

Adjust front side door as needed. Refer to Front Side Door Adjustment.